 -- Copyright (C) 1991-2010 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (1.5V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --					Bank 1:		3.3V
 --					Bank 2:		1.5V
 --					Bank 3:		2.5V
 --					Bank 4:		2.5V
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   For transceiver I/O banks, connect each pin marked GND*
 --           	    either individually through a 10k Ohm resistor to GND or tie all pins
 --           	    together and connect through a single 10k Ohm resistor to GND.
 --           	    For non-transceiver I/O banks, connect each pin marked GND* directly to GND
 --           	    or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II Version 9.1 Build 350 03/24/2010 Service Pack 2 SJ Web Edition
CHIP  "Skiroc2"  ASSIGNED TO AN: EP1C6Q240C6

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
adc_clk                      : 1         : output : 3.3-V LVTTL       :         : 1         : Y              
SYNC_GENE                    : 2         : output : 3.3-V LVTTL       :         : 1         : Y              
RESERVED_INPUT               : 3         :        :                   :         : 1         :                
RESERVED_INPUT               : 4         :        :                   :         : 1         :                
DAQ11                        : 5         : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ12                        : 6         : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ9                         : 7         : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ10                        : 8         : bidir  : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : 9         : power  :                   : 3.3V    : 1         :                
GND                          : 10        : gnd    :                   :         :           :                
DAQ7                         : 11        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ8                         : 12        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ5                         : 13        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ6                         : 14        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ3                         : 15        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ4                         : 16        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ1                         : 17        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ2                         : 18        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DAQ0                         : 19        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
RESERVED_INPUT               : 20        :        :                   :         : 1         :                
start_acq                    : 21        : output : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : 22        : power  :                   : 3.3V    : 1         :                
RESERVED_INPUT               : 23        :        :                   :         : 1         :                
~nCSO~ / RESERVED_INPUT      : 24        : input  : 3.3-V LVTTL       :         : 1         : N              
DATA0                        : 25        : input  :                   :         : 1         :                
nCONFIG                      : 26        :        :                   :         : 1         :                
VCCA_PLL1                    : 27        : power  :                   : 1.5V    :           :                
clk_osc                      : 28        : input  : 3.3-V LVTTL       :         : 1         : Y              
GND+                         : 29        :        :                   :         : 1         :                
GNDA_PLL1                    : 30        : gnd    :                   :         :           :                
GNDG_PLL1                    : 31        : gnd    :                   :         :           :                
nCEO                         : 32        :        :                   :         : 1         :                
nCE                          : 33        :        :                   :         : 1         :                
MSEL0                        : 34        :        :                   :         : 1         :                
MSEL1                        : 35        :        :                   :         : 1         :                
DCLK                         : 36        : bidir  :                   :         : 1         :                
~ASDO~ / RESERVED_INPUT      : 37        : input  : 3.3-V LVTTL       :         : 1         : N              
PLL_OUT                      : 38        : output : 3.3-V LVTTL       :         : 1         : Y              
RESERVED_INPUT               : 39        :        :                   :         : 1         :                
GND                          : 40        : gnd    :                   :         :           :                
rstb_pa                      : 41        : output : 3.3-V LVTTL       :         : 1         : Y              
ck_read                      : 42        : output : 3.3-V LVTTL       :         : 1         : Y              
srin_read                    : 43        : output : 3.3-V LVTTL       :         : 1         : Y              
pwr_on_a                     : 44        : output : 3.3-V LVTTL       :         : 1         : Y              
pwr_on_adc                   : 45        : output : 3.3-V LVTTL       :         : 1         : Y              
pwr_on_dac                   : 46        : output : 3.3-V LVTTL       :         : 1         : Y              
pwr_on_d                     : 47        : output : 3.3-V LVTTL       :         : 1         : Y              
sr_in                        : 48        : output : 3.3-V LVTTL       :         : 1         : Y              
sr_rstb                      : 49        : output : 3.3-V LVTTL       :         : 1         : Y              
sr_ck                        : 50        : output : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : 51        : power  :                   : 3.3V    : 1         :                
GND                          : 52        : gnd    :                   :         :           :                
select                       : 53        : output : 3.3-V LVTTL       :         : 1         : Y              
resetb                       : 54        : output : 3.3-V LVTTL       :         : 1         : Y              
start_readout1               : 55        : output : 3.3-V LVTTL       :         : 1         : Y              
start_readout2               : 56        : output : 3.3-V LVTTL       :         : 1         : Y              
start_convb                  : 57        : output : 3.3-V LVTTL       :         : 1         : Y              
40M_test                     : 58        : output : 3.3-V LVTTL       :         : 1         : Y              
start_rampb_adc_ext          : 59        : output : 3.3-V LVTTL       :         : 1         : Y              
start_ramp_tdc_ext           : 60        : output : 3.3-V LVTTL       :         : 1         : Y              
LED                          : 61        : output : 2.5 V             :         : 4         : Y              
RESERVED_INPUT               : 62        :        :                   :         : 4         :                
RESERVED_INPUT               : 63        :        :                   :         : 4         :                
RESERVED_INPUT               : 64        :        :                   :         : 4         :                
RESERVED_INPUT               : 65        :        :                   :         : 4         :                
RESERVED_INPUT               : 66        :        :                   :         : 4         :                
srout_read                   : 67        : input  : 3.3-V LVTTL       :         : 4         : Y              
sr_out                       : 68        : input  : 3.3-V LVTTL       :         : 4         : Y              
GND                          : 69        : gnd    :                   :         :           :                
VCCIO4                       : 70        : power  :                   : 2.5V    : 4         :                
GND                          : 71        : gnd    :                   :         :           :                
VCCINT                       : 72        : power  :                   : 1.5V    :           :                
digital_probe1               : 73        : input  : 3.3-V LVTTL       :         : 4         : Y              
digital_probe2               : 74        : input  : 3.3-V LVTTL       :         : 4         : Y              
end_readout1                 : 75        : input  : 3.3-V LVTTL       :         : 4         : Y              
end_readout2                 : 76        : input  : 3.3-V LVTTL       :         : 4         : Y              
RESERVED_INPUT               : 77        :        :                   :         : 4         :                
RESERVED_INPUT               : 78        :        :                   :         : 4         :                
RESERVED_INPUT               : 79        :        :                   :         : 4         :                
RESERVED_INPUT               : 80        :        :                   :         : 4         :                
RESERVED_INPUT               : 81        :        :                   :         : 4         :                
5M                           : 82        : output : LVDS              :         : 4         : Y              
5M(n)                        : 83        : output : LVDS              :         : 4         : Y              
RESERVED_INPUT               : 84        :        :                   :         : 4         :                
RESERVED_INPUT               : 85        :        :                   :         : 4         :                
40M                          : 86        : output : LVDS              :         : 4         : Y              
40M(n)                       : 87        : output : LVDS              :         : 4         : Y              
RESERVED_INPUT               : 88        :        :                   :         : 4         :                
GND                          : 89        : gnd    :                   :         :           :                
VCCINT                       : 90        : power  :                   : 1.5V    :           :                
GND                          : 91        : gnd    :                   :         :           :                
VCCIO4                       : 92        : power  :                   : 2.5V    : 4         :                
RESERVED_INPUT               : 93        :        :                   :         : 4         :                
RESERVED_INPUT               : 94        :        :                   :         : 4         :                
RESERVED_INPUT               : 95        :        :                   :         : 4         :                
V_E                          : 96        : output : LVDS              :         : 4         : Y              
V_E(n)                       : 97        : output : LVDS              :         : 4         : Y              
RESERVED_INPUT               : 98        :        :                   :         : 4         :                
RESERVED_INPUT               : 99        :        :                   :         : 4         :                
T_E                          : 100       : output : LVDS              :         : 4         : Y              
T_E(n)                       : 101       : output : LVDS              :         : 4         : Y              
RESERVED_INPUT               : 102       :        :                   :         : 4         :                
RESERVED_INPUT               : 103       :        :                   :         : 4         :                
R_C                          : 104       : output : LVDS              :         : 4         : Y              
R_C(n)                       : 105       : output : LVDS              :         : 4         : Y              
RESERVED_INPUT               : 106       :        :                   :         : 4         :                
RESERVED_INPUT               : 107       :        :                   :         : 4         :                
RESERVED_INPUT               : 108       :        :                   :         : 4         :                
GND                          : 109       : gnd    :                   :         :           :                
VCCINT                       : 110       : power  :                   : 1.5V    :           :                
GND                          : 111       : gnd    :                   :         :           :                
VCCIO4                       : 112       : power  :                   : 2.5V    : 4         :                
RESERVED_INPUT               : 113       :        :                   :         : 4         :                
RESERVED_INPUT               : 114       :        :                   :         : 4         :                
ChipSatb                     : 115       : input  : 2.5 V             :         : 4         : Y              
TransmitOn1b                 : 116       : input  : 2.5 V             :         : 4         : Y              
TransmitOn2b                 : 117       : input  : 2.5 V             :         : 4         : Y              
Dout1b                       : 118       : input  : 2.5 V             :         : 4         : Y              
Dout2b                       : 119       : input  : 2.5 V             :         : 4         : Y              
TrigOutb                     : 120       : input  : 2.5 V             :         : 4         : Y              
pwr_reset                    : 121       : input  : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT               : 122       :        :                   :         : 3         :                
RESERVED_INPUT               : 123       :        :                   :         : 3         :                
OTR                          : 124       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[11]                      : 125       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[10]                      : 126       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[9]                       : 127       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[8]                       : 128       : input  : 3.3-V LVTTL       :         : 3         : Y              
GND                          : 129       : gnd    :                   :         :           :                
VCCIO3                       : 130       : power  :                   : 2.5V    : 3         :                
ADC[7]                       : 131       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[6]                       : 132       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[5]                       : 133       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[4]                       : 134       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[3]                       : 135       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[2]                       : 136       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[1]                       : 137       : input  : 3.3-V LVTTL       :         : 3         : Y              
ADC[0]                       : 138       : input  : 3.3-V LVTTL       :         : 3         : Y              
RESERVED_INPUT               : 139       :        :                   :         : 3         :                
RESERVED_INPUT               : 140       :        :                   :         : 3         :                
RESERVED_INPUT               : 141       :        :                   :         : 3         :                
GND                          : 142       : gnd    :                   :         :           :                
RESERVED_INPUT               : 143       :        :                   :         : 3         :                
out_altera1                  : 144       : output : 2.5 V             :         : 3         : Y              
CONF_DONE                    : 145       :        :                   :         : 3         :                
nSTATUS                      : 146       :        :                   :         : 3         :                
TCK                          : 147       : input  :                   :         : 3         :                
TMS                          : 148       : input  :                   :         : 3         :                
TDO                          : 149       : output :                   :         : 3         :                
GNDG_PLL2                    : 150       : gnd    :                   :         :           :                
GNDA_PLL2                    : 151       : gnd    :                   :         :           :                
GND+                         : 152       :        :                   :         : 3         :                
GND+                         : 153       :        :                   :         : 3         :                
VCCA_PLL2                    : 154       : power  :                   : 1.5V    :           :                
TDI                          : 155       : input  :                   :         : 3         :                
out_altera2                  : 156       : output : 2.5 V             :         : 3         : Y              
VCCIO3                       : 157       : power  :                   : 2.5V    : 3         :                
out_altera3                  : 158       : output : 2.5 V             :         : 3         : Y              
out_altera4                  : 159       : output : 2.5 V             :         : 3         : Y              
out_altera5                  : 160       : output : 2.5 V             :         : 3         : Y              
out_altera6                  : 161       : output : 2.5 V             :         : 3         : Y              
RESERVED_INPUT               : 162       :        :                   :         : 3         :                
nRXF                         : 163       : input  : 2.5 V             :         : 3         : Y              
nTXE                         : 164       : input  : 2.5 V             :         : 3         : Y              
WR                           : 165       : output : 2.5 V             :         : 3         : Y              
nRD                          : 166       : output : 2.5 V             :         : 3         : Y              
USB[3]                       : 167       : bidir  : 2.5 V             :         : 3         : Y              
USB[6]                       : 168       : bidir  : 2.5 V             :         : 3         : Y              
USB[5]                       : 169       : bidir  : 2.5 V             :         : 3         : Y              
USB[7]                       : 170       : bidir  : 2.5 V             :         : 3         : Y              
GND                          : 171       : gnd    :                   :         :           :                
VCCIO3                       : 172       : power  :                   : 2.5V    : 3         :                
USB[1]                       : 173       : bidir  : 2.5 V             :         : 3         : Y              
USB[2]                       : 174       : bidir  : 2.5 V             :         : 3         : Y              
USB[4]                       : 175       : bidir  : 2.5 V             :         : 3         : Y              
USB[0]                       : 176       : bidir  : 2.5 V             :         : 3         : Y              
XTIN                         : 177       : input  : 2.5 V             :         : 3         : Y              
RESERVED_INPUT               : 178       :        :                   :         : 3         :                
test40                       : 179       : output : 2.5 V             :         : 3         : Y              
test39                       : 180       : output : 2.5 V             :         : 3         : Y              
test38                       : 181       : output : 1.5 V             :         : 2         : Y              
test37                       : 182       : output : 1.5 V             :         : 2         : Y              
test36                       : 183       : output : 1.5 V             :         : 2         : Y              
test35                       : 184       : output : 1.5 V             :         : 2         : Y              
test34                       : 185       : output : 1.5 V             :         : 2         : Y              
test33                       : 186       : output : 1.5 V             :         : 2         : Y              
test32                       : 187       : output : 1.5 V             :         : 2         : Y              
test31                       : 188       : output : 1.5 V             :         : 2         : Y              
VCCIO2                       : 189       : power  :                   : 1.5V    : 2         :                
GND                          : 190       : gnd    :                   :         :           :                
VCCINT                       : 191       : power  :                   : 1.5V    :           :                
GND                          : 192       : gnd    :                   :         :           :                
test30                       : 193       : output : 1.5 V             :         : 2         : Y              
test29                       : 194       : output : 1.5 V             :         : 2         : Y              
test28                       : 195       : output : 1.5 V             :         : 2         : Y              
test27                       : 196       : output : 1.5 V             :         : 2         : Y              
test26                       : 197       : output : 1.5 V             :         : 2         : Y              
test25                       : 198       : output : 1.5 V             :         : 2         : Y              
test24                       : 199       : output : 1.5 V             :         : 2         : Y              
test23                       : 200       : output : 1.5 V             :         : 2         : Y              
test22                       : 201       : output : 1.5 V             :         : 2         : Y              
test21                       : 202       : output : 1.5 V             :         : 2         : Y              
test20                       : 203       : output : 1.5 V             :         : 2         : Y              
test19                       : 204       : output : 1.5 V             :         : 2         : Y              
test18                       : 205       : output : 1.5 V             :         : 2         : Y              
test17                       : 206       : output : 1.5 V             :         : 2         : Y              
test16                       : 207       : output : 1.5 V             :         : 2         : Y              
RESERVED_INPUT               : 208       :        :                   :         : 2         :                
VCCIO2                       : 209       : power  :                   : 1.5V    : 2         :                
GND                          : 210       : gnd    :                   :         :           :                
VCCINT                       : 211       : power  :                   : 1.5V    :           :                
GND                          : 212       : gnd    :                   :         :           :                
test15                       : 213       : output : 1.5 V             :         : 2         : Y              
test14                       : 214       : output : 1.5 V             :         : 2         : Y              
test13                       : 215       : output : 1.5 V             :         : 2         : Y              
test12                       : 216       : output : 1.5 V             :         : 2         : Y              
test11                       : 217       : output : 1.5 V             :         : 2         : Y              
test10                       : 218       : output : 1.5 V             :         : 2         : Y              
test9                        : 219       : output : 1.5 V             :         : 2         : Y              
IN_ALTERA6                   : 220       : input  : 1.5 V             :         : 2         : Y              
test8                        : 221       : output : 1.5 V             :         : 2         : Y              
IN_ALTERA5                   : 222       : input  : 1.5 V             :         : 2         : Y              
test7                        : 223       : output : 1.5 V             :         : 2         : Y              
IN_ALTERA4                   : 224       : input  : 1.5 V             :         : 2         : Y              
test6                        : 225       : output : 1.5 V             :         : 2         : Y              
IN_ALTERA3                   : 226       : input  : 1.5 V             :         : 2         : Y              
test5                        : 227       : output : 1.5 V             :         : 2         : Y              
IN_ALTERA2                   : 228       : input  : 1.5 V             :         : 2         : Y              
VCCINT                       : 229       : power  :                   : 1.5V    :           :                
GND                          : 230       : gnd    :                   :         :           :                
VCCIO2                       : 231       : power  :                   : 1.5V    : 2         :                
GND                          : 232       : gnd    :                   :         :           :                
test4                        : 233       : output : 1.5 V             :         : 2         : Y              
IN_ALTERA1                   : 234       : input  : 1.5 V             :         : 2         : Y              
test3                        : 235       : output : 1.5 V             :         : 2         : Y              
hold_conn                    : 236       : input  : 1.5 V             :         : 2         : Y              
test2                        : 237       : output : 1.5 V             :         : 2         : Y              
clk_gene_ext                 : 238       : input  : 1.5 V             :         : 2         : Y              
test1                        : 239       : output : 1.5 V             :         : 2         : Y              
hold                         : 240       : output : 1.5 V             :         : 2         : Y              
