# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2010 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II
# Version 10.0 Build 262 08/18/2010 Service Pack 1 SJ Web Edition
# Date created = 18:47:10  October 12, 2010
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		Skiroc2_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY Cyclone
set_global_assignment -name DEVICE EP1C6Q240C6
set_global_assignment -name TOP_LEVEL_ENTITY Skiroc2
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "10.0 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "18:47:10  OCTOBER 12, 2010"
set_global_assignment -name LAST_QUARTUS_VERSION "9.1 SP2"
set_global_assignment -name DEVICE_FILTER_PACKAGE PQFP
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 240
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD "3.3-V LVTTL"
set_location_assignment PIN_61 -to LED
set_location_assignment PIN_226 -to IN_ALTERA3
set_global_assignment -name WEAK_PULL_UP_RESISTOR OFF
set_global_assignment -name SYNTH_TIMING_DRIVEN_SYNTHESIS OFF
set_global_assignment -name ENABLE_LOGIC_ANALYZER_INTERFACE OFF
set_location_assignment PIN_234 -to IN_ALTERA1
set_location_assignment PIN_228 -to IN_ALTERA2
set_location_assignment PIN_224 -to IN_ALTERA4
set_location_assignment PIN_222 -to IN_ALTERA5
set_location_assignment PIN_220 -to IN_ALTERA6
set_location_assignment PIN_1 -to adc_clk
set_location_assignment PIN_42 -to ck_read
set_location_assignment PIN_44 -to pwr_on_a
set_location_assignment PIN_45 -to pwr_on_adc
set_location_assignment PIN_47 -to pwr_on_d
set_location_assignment PIN_46 -to pwr_on_dac
set_location_assignment PIN_54 -to resetb
set_location_assignment PIN_41 -to rstb_pa
set_location_assignment PIN_53 -to select
set_location_assignment PIN_50 -to sr_ck
set_location_assignment PIN_48 -to sr_in
set_location_assignment PIN_49 -to sr_rstb
set_location_assignment PIN_43 -to srin_read
set_location_assignment PIN_58 -to 40M_test
set_location_assignment PIN_21 -to start_acq
set_location_assignment PIN_57 -to start_convb
set_location_assignment PIN_60 -to start_ramp_tdc_ext
set_location_assignment PIN_59 -to start_rampb_adc_ext
set_location_assignment PIN_55 -to start_readout1
set_location_assignment PIN_56 -to start_readout2
set_location_assignment PIN_2 -to SYNC_GENE
set_location_assignment PIN_144 -to out_altera1
set_location_assignment PIN_156 -to out_altera2
set_location_assignment PIN_158 -to out_altera3
set_location_assignment PIN_159 -to out_altera4
set_location_assignment PIN_160 -to out_altera5
set_location_assignment PIN_161 -to out_altera6
set_location_assignment PIN_166 -to nRD
set_location_assignment PIN_188 -to test31
set_location_assignment PIN_187 -to test32
set_location_assignment PIN_186 -to test33
set_location_assignment PIN_185 -to test34
set_location_assignment PIN_184 -to test35
set_location_assignment PIN_183 -to test36
set_location_assignment PIN_182 -to test37
set_location_assignment PIN_181 -to test38
set_location_assignment PIN_180 -to test39
set_location_assignment PIN_179 -to test40
set_location_assignment PIN_165 -to WR
set_instance_assignment -name IO_STANDARD LVDS -to 40M
set_instance_assignment -name IO_STANDARD LVDS -to 5M
set_instance_assignment -name IO_STANDARD LVDS -to R_C
set_instance_assignment -name IO_STANDARD LVDS -to T_E
set_instance_assignment -name IO_STANDARD "2.5 V" -to WR
set_instance_assignment -name IO_STANDARD LVDS -to V_E
set_location_assignment PIN_240 -to hold
set_location_assignment PIN_239 -to test1
set_location_assignment PIN_237 -to test2
set_location_assignment PIN_235 -to test3
set_location_assignment PIN_233 -to test4
set_location_assignment PIN_227 -to test5
set_location_assignment PIN_225 -to test6
set_location_assignment PIN_223 -to test7
set_location_assignment PIN_221 -to test8
set_location_assignment PIN_219 -to test9
set_location_assignment PIN_218 -to test10
set_location_assignment PIN_217 -to test11
set_location_assignment PIN_216 -to test12
set_location_assignment PIN_215 -to test13
set_location_assignment PIN_214 -to test14
set_location_assignment PIN_213 -to test15
set_location_assignment PIN_207 -to test16
set_location_assignment PIN_206 -to test17
set_location_assignment PIN_205 -to test18
set_location_assignment PIN_204 -to test19
set_location_assignment PIN_203 -to test20
set_location_assignment PIN_202 -to test21
set_location_assignment PIN_201 -to test22
set_location_assignment PIN_200 -to test23
set_location_assignment PIN_199 -to test24
set_location_assignment PIN_198 -to test25
set_location_assignment PIN_197 -to test26
set_location_assignment PIN_196 -to test27
set_location_assignment PIN_195 -to test28
set_location_assignment PIN_194 -to test29
set_location_assignment PIN_193 -to test30
set_location_assignment PIN_82 -to 5M
set_location_assignment PIN_83 -to "5M(n)"
set_location_assignment PIN_86 -to 40M
set_location_assignment PIN_87 -to "40M(n)"
set_location_assignment PIN_104 -to R_C
set_location_assignment PIN_105 -to "R_C(n)"
set_location_assignment PIN_100 -to T_E
set_location_assignment PIN_101 -to "T_E(n)"
set_location_assignment PIN_96 -to V_E
set_location_assignment PIN_97 -to "V_E(n)"
set_instance_assignment -name IO_STANDARD "2.5 V" -to LED
set_instance_assignment -name IO_STANDARD "2.5 V" -to out_altera1
set_instance_assignment -name IO_STANDARD "2.5 V" -to out_altera2
set_instance_assignment -name IO_STANDARD "2.5 V" -to out_altera3
set_instance_assignment -name IO_STANDARD "2.5 V" -to out_altera4
set_instance_assignment -name IO_STANDARD "2.5 V" -to out_altera5
set_instance_assignment -name IO_STANDARD "2.5 V" -to out_altera6
set_instance_assignment -name IO_STANDARD "2.5 V" -to nRD
set_instance_assignment -name IO_STANDARD "2.5 V" -to test40
set_instance_assignment -name IO_STANDARD "2.5 V" -to test39
set_instance_assignment -name IO_STANDARD "1.5 V" -to test38
set_instance_assignment -name IO_STANDARD "1.5 V" -to test37
set_instance_assignment -name IO_STANDARD "1.5 V" -to test36
set_instance_assignment -name IO_STANDARD "1.5 V" -to test35
set_instance_assignment -name IO_STANDARD "1.5 V" -to test34
set_instance_assignment -name IO_STANDARD "1.5 V" -to test33
set_instance_assignment -name IO_STANDARD "1.5 V" -to test32
set_instance_assignment -name IO_STANDARD "1.5 V" -to test31
set_instance_assignment -name IO_STANDARD "1.5 V" -to test30
set_instance_assignment -name IO_STANDARD "1.5 V" -to test29
set_instance_assignment -name IO_STANDARD "1.5 V" -to test28
set_instance_assignment -name IO_STANDARD "1.5 V" -to test27
set_instance_assignment -name IO_STANDARD "1.5 V" -to test26
set_instance_assignment -name IO_STANDARD "1.5 V" -to test25
set_instance_assignment -name IO_STANDARD "1.5 V" -to test24
set_instance_assignment -name IO_STANDARD "1.5 V" -to test23
set_instance_assignment -name IO_STANDARD "1.5 V" -to test22
set_instance_assignment -name IO_STANDARD "1.5 V" -to test21
set_instance_assignment -name IO_STANDARD "1.5 V" -to test20
set_instance_assignment -name IO_STANDARD "1.5 V" -to test19
set_instance_assignment -name IO_STANDARD "1.5 V" -to test18
set_instance_assignment -name IO_STANDARD "1.5 V" -to test17
set_instance_assignment -name IO_STANDARD "1.5 V" -to test16
set_instance_assignment -name IO_STANDARD "1.5 V" -to test15
set_instance_assignment -name IO_STANDARD "1.5 V" -to test14
set_instance_assignment -name IO_STANDARD "1.5 V" -to test13
set_instance_assignment -name IO_STANDARD "1.5 V" -to test12
set_instance_assignment -name IO_STANDARD "1.5 V" -to test11
set_instance_assignment -name IO_STANDARD "1.5 V" -to test10
set_instance_assignment -name IO_STANDARD "1.5 V" -to test9
set_instance_assignment -name IO_STANDARD "1.5 V" -to IN_ALTERA6
set_instance_assignment -name IO_STANDARD "1.5 V" -to test8
set_instance_assignment -name IO_STANDARD "1.5 V" -to IN_ALTERA5
set_instance_assignment -name IO_STANDARD "1.5 V" -to test7
set_instance_assignment -name IO_STANDARD "1.5 V" -to IN_ALTERA4
set_instance_assignment -name IO_STANDARD "1.5 V" -to test6
set_instance_assignment -name IO_STANDARD "1.5 V" -to IN_ALTERA3
set_instance_assignment -name IO_STANDARD "1.5 V" -to test5
set_instance_assignment -name IO_STANDARD "1.5 V" -to IN_ALTERA2
set_instance_assignment -name IO_STANDARD "1.5 V" -to test4
set_instance_assignment -name IO_STANDARD "1.5 V" -to IN_ALTERA1
set_instance_assignment -name IO_STANDARD "1.5 V" -to test3
set_instance_assignment -name IO_STANDARD "1.5 V" -to test2
set_instance_assignment -name IO_STANDARD "1.5 V" -to test1
set_instance_assignment -name IO_STANDARD "1.5 V" -to hold
set_location_assignment PIN_176 -to USB[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[0]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[7]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[6]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[5]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[4]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[3]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[2]
set_instance_assignment -name IO_STANDARD "2.5 V" -to USB[1]
set_location_assignment PIN_175 -to USB[4]
set_location_assignment PIN_174 -to USB[2]
set_location_assignment PIN_167 -to USB[3]
set_location_assignment PIN_173 -to USB[1]
set_location_assignment PIN_170 -to USB[7]
set_location_assignment PIN_168 -to USB[6]
set_location_assignment PIN_169 -to USB[5]
set_location_assignment PIN_19 -to DAQ0
set_location_assignment PIN_18 -to DAQ2
set_location_assignment PIN_17 -to DAQ1
set_location_assignment PIN_16 -to DAQ4
set_location_assignment PIN_15 -to DAQ3
set_location_assignment PIN_14 -to DAQ6
set_location_assignment PIN_13 -to DAQ5
set_location_assignment PIN_11 -to DAQ7
set_location_assignment PIN_12 -to DAQ8
set_location_assignment PIN_8 -to DAQ10
set_location_assignment PIN_7 -to DAQ9
set_location_assignment PIN_5 -to DAQ11
set_location_assignment PIN_6 -to DAQ12
set_location_assignment PIN_28 -to clk_osc
set_location_assignment PIN_73 -to digital_probe1
set_location_assignment PIN_74 -to digital_probe2
set_location_assignment PIN_75 -to end_readout1
set_location_assignment PIN_76 -to end_readout2
set_location_assignment PIN_67 -to srout_read
set_location_assignment PIN_68 -to sr_out
set_location_assignment PIN_116 -to TransmitOn1b
set_location_assignment PIN_117 -to TransmitOn2b
set_location_assignment PIN_120 -to TrigOutb
set_location_assignment PIN_118 -to Dout1b
set_location_assignment PIN_119 -to Dout2b
set_location_assignment PIN_124 -to OTR
set_location_assignment PIN_125 -to ADC[11]
set_location_assignment PIN_126 -to ADC[10]
set_location_assignment PIN_127 -to ADC[9]
set_location_assignment PIN_128 -to ADC[8]
set_location_assignment PIN_131 -to ADC[7]
set_location_assignment PIN_132 -to ADC[6]
set_location_assignment PIN_133 -to ADC[5]
set_location_assignment PIN_134 -to ADC[4]
set_location_assignment PIN_135 -to ADC[3]
set_location_assignment PIN_136 -to ADC[2]
set_location_assignment PIN_137 -to ADC[1]
set_location_assignment PIN_138 -to ADC[0]
set_location_assignment PIN_163 -to nRXF
set_location_assignment PIN_164 -to nTXE
set_location_assignment PIN_38 -to PLL_OUT
set_location_assignment PIN_177 -to XTIN
set_location_assignment PIN_238 -to clk_gene_ext
set_instance_assignment -name IO_STANDARD "2.5 V" -to nTXE
set_instance_assignment -name IO_STANDARD "2.5 V" -to nRXF
set_instance_assignment -name IO_STANDARD "2.5 V" -to XTIN
set_instance_assignment -name IO_STANDARD "2.5 V" -to TransmitOn1b
set_instance_assignment -name IO_STANDARD "2.5 V" -to TransmitOn2b
set_instance_assignment -name IO_STANDARD "2.5 V" -to Dout1b
set_instance_assignment -name IO_STANDARD "2.5 V" -to Dout2b
set_instance_assignment -name IO_STANDARD "2.5 V" -to TrigOutb
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to OTR
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to ADC[0]
set_instance_assignment -name IO_STANDARD "1.5 V" -to clk_gene_ext
set_global_assignment -name FLOW_ENABLE_IO_ASSIGNMENT_ANALYSIS ON
set_global_assignment -name SAVE_DISK_SPACE OFF
set_location_assignment PIN_115 -to ChipSatb
set_instance_assignment -name IO_STANDARD "2.5 V" -to ChipSatb
set_location_assignment PIN_121 -to pwr_reset
set_location_assignment PIN_236 -to hold_conn
set_instance_assignment -name IO_STANDARD "1.5 V" -to hold_conn
set_global_assignment -name RESERVE_ALL_UNUSED_PINS "AS INPUT TRI-STATED"
set_global_assignment -name RESERVE_ASDO_AFTER_CONFIGURATION "AS INPUT TRI-STATED"
set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"
set_global_assignment -name LL_ROOT_REGION ON -section_id "Root Region"
set_global_assignment -name LL_MEMBER_STATE LOCKED -section_id "Root Region"
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top
set_global_assignment -name SEARCH_PATH "AutoDAQ/VHDL ONLY/" -tag from_archive
set_global_assignment -name SEARCH_PATH usb_fw_v23_verilog/ -tag from_archive
set_global_assignment -name MISC_FILE Skiroc2.dpf
set_global_assignment -name BDF_FILE Skiroc2.bdf
set_global_assignment -name VHDL_FILE SlowControl_SK2_ERO_v3.vhd
set_global_assignment -name QIP_FILE pll_sk2.qip
set_global_assignment -name VERILOG_FILE usb_fw_v23_verilog/usb_full_interface_v.v
set_global_assignment -name VERILOG_FILE usb_fw_v23_verilog/interruptunit.v
set_global_assignment -name VERILOG_FILE usb_fw_v23_verilog/readrequnit.v
set_global_assignment -name VERILOG_FILE usb_fw_v23_verilog/rxunit.v
set_global_assignment -name VERILOG_FILE usb_fw_v23_verilog/txunit.v
set_global_assignment -name VHDL_FILE Firmware_version.vhd
set_global_assignment -name VHDL_FILE Read_TransmitData_SK2.vhd
set_global_assignment -name VHDL_FILE Enable_sync_clock.vhd
set_global_assignment -name QIP_FILE clk_div.qip
set_global_assignment -name QIP_FILE ck_mux.qip
set_global_assignment -name VHDL_FILE latch_8.vhd
set_global_assignment -name VHDL_FILE Read_Word.vhd
set_global_assignment -name VHDL_FILE AutoDAQ_SK2_v1.vhd
set_global_assignment -name VHDL_FILE Scurve_1input_16bits_SK2.vhd
set_global_assignment -name VHDL_FILE RSwithTimeOut.vhd
set_global_assignment -name QIP_FILE fifo.qip
set_global_assignment -name QIP_FILE flipflop.qip
set_global_assignment -name QIP_FILE flipflopaclr.qip
set_global_assignment -name QIP_FILE flipflopaclr_en.qip
set_global_assignment -name QIP_FILE count4bits.qip
set_global_assignment -name QIP_FILE reg_8bits.qip
set_global_assignment -name QIP_FILE data_count.qip
set_global_assignment -name QIP_FILE big_fifo.qip
set_global_assignment -name QIP_FILE shift8register.qip
set_global_assignment -name QIP_FILE count16bits.qip
set_global_assignment -name QIP_FILE fifo_adc.qip
set_global_assignment -name QIP_FILE counter_10b.qip
set_global_assignment -name QIP_FILE delay_OR_trigger.qip
set_global_assignment -name QIP_FILE delay_mux.qip
set_global_assignment -name QIP_FILE count4timeout.qip
set_global_assignment -name VHDL_FILE static_8bit_registers.vhd
set_global_assignment -name QIP_FILE mux4_1.qip
set_global_assignment -name QIP_FILE count27bits.qip
set_global_assignment -name VHDL_FILE External_ADC_SK2CMS.vhd
set_global_assignment -name VHDL_FILE External_ADC_SK2_v2.vhd
set_global_assignment -name QIP_FILE fifo_acd_SK2CMS.qip
set_global_assignment -name QIP_FILE count2bits.qip
set_global_assignment -name VHDL_FILE AutoDAQ_SK2CMS_v1a.vhd
set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top
set_global_assignment -name INCREMENTAL_COMPILATION OFF