Fitter report for Skiroc2
Mon Apr 30 15:17:38 2018
Quartus II Version 9.1 Build 350 03/24/2010 Service Pack 2 SJ Web Edition


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Fitter Summary
  3. Fitter Settings
  4. Parallel Compilation
  5. Pin-Out File
  6. Fitter Resource Usage Summary
  7. Input Pins
  8. Output Pins
  9. Bidir Pins
 10. I/O Bank Usage
 11. All Package Pins
 12. PLL Summary
 13. PLL Usage
 14. Output Pin Default Load For Reported TCO
 15. Fitter Resource Utilization by Entity
 16. Delay Chain Summary
 17. Pad To Core Delay Chain Fanout
 18. Control Signals
 19. Global & Other Fast Signals
 20. Non-Global High Fan-Out Signals
 21. Fitter RAM Summary
 22. Interconnect Usage Summary
 23. LAB Logic Elements
 24. LAB-wide Signals
 25. LAB Signals Sourced
 26. LAB Signals Sourced Out
 27. LAB Distinct Inputs
 28. Fitter Device Options
 29. Estimated Delay Added for Hold Timing
 30. Fitter Messages
 31. Fitter Suppressed Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2010 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.



+----------------------------------------------------------------------+
; Fitter Summary                                                       ;
+-----------------------+----------------------------------------------+
; Fitter Status         ; Successful - Mon Apr 30 15:17:38 2018        ;
; Quartus II Version    ; 9.1 Build 350 03/24/2010 SP 2 SJ Web Edition ;
; Revision Name         ; Skiroc2                                      ;
; Top-level Entity Name ; Skiroc2                                      ;
; Family                ; Cyclone                                      ;
; Device                ; EP1C6Q240C6                                  ;
; Timing Models         ; Final                                        ;
; Total logic elements  ; 2,431 / 5,980 ( 41 % )                       ;
; Total pins            ; 141 / 185 ( 76 % )                           ;
; Total virtual pins    ; 0                                            ;
; Total memory bits     ; 67,584 / 92,160 ( 73 % )                     ;
; Total PLLs            ; 1 / 2 ( 50 % )                               ;
+-----------------------+----------------------------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Settings                                                                                                                              ;
+----------------------------------------------------------------------------+--------------------------------+--------------------------------+
; Option                                                                     ; Setting                        ; Default Value                  ;
+----------------------------------------------------------------------------+--------------------------------+--------------------------------+
; Device                                                                     ; EP1C6Q240C6                    ;                                ;
; Fit Attempts to Skip                                                       ; 0                              ; 0.0                            ;
; Device I/O Standard                                                        ; 3.3-V LVTTL                    ;                                ;
; Use smart compilation                                                      ; Off                            ; Off                            ;
; Enable parallel Assembler and TimeQuest Timing Analyzer during compilation ; On                             ; On                             ;
; Enable compact report table                                                ; Off                            ; Off                            ;
; Use TimeQuest Timing Analyzer                                              ; Off                            ; Off                            ;
; Router Timing Optimization Level                                           ; Normal                         ; Normal                         ;
; Placement Effort Multiplier                                                ; 1.0                            ; 1.0                            ;
; Router Effort Multiplier                                                   ; 1.0                            ; 1.0                            ;
; Optimize Hold Timing                                                       ; IO Paths and Minimum TPD Paths ; IO Paths and Minimum TPD Paths ;
; Optimize Multi-Corner Timing                                               ; Off                            ; Off                            ;
; Optimize Timing                                                            ; Normal compilation             ; Normal compilation             ;
; Optimize Timing for ECOs                                                   ; Off                            ; Off                            ;
; Regenerate full fit report during ECO compiles                             ; Off                            ; Off                            ;
; Optimize IOC Register Placement for Timing                                 ; On                             ; On                             ;
; Limit to One Fitting Attempt                                               ; Off                            ; Off                            ;
; Final Placement Optimizations                                              ; Automatically                  ; Automatically                  ;
; Fitter Aggressive Routability Optimizations                                ; Automatically                  ; Automatically                  ;
; Fitter Initial Placement Seed                                              ; 1                              ; 1                              ;
; Slow Slew Rate                                                             ; Off                            ; Off                            ;
; PCI I/O                                                                    ; Off                            ; Off                            ;
; Weak Pull-Up Resistor                                                      ; Off                            ; Off                            ;
; Enable Bus-Hold Circuitry                                                  ; Off                            ; Off                            ;
; Auto Global Memory Control Signals                                         ; Off                            ; Off                            ;
; Auto Packed Registers                                                      ; Auto                           ; Auto                           ;
; Auto Delay Chains                                                          ; On                             ; On                             ;
; Auto Merge PLLs                                                            ; On                             ; On                             ;
; Perform Physical Synthesis for Combinational Logic for Performance         ; Off                            ; Off                            ;
; Perform Register Duplication for Performance                               ; Off                            ; Off                            ;
; Perform Register Retiming for Performance                                  ; Off                            ; Off                            ;
; Perform Asynchronous Signal Pipelining                                     ; Off                            ; Off                            ;
; Fitter Effort                                                              ; Auto Fit                       ; Auto Fit                       ;
; Physical Synthesis Effort Level                                            ; Normal                         ; Normal                         ;
; Logic Cell Insertion - Logic Duplication                                   ; Auto                           ; Auto                           ;
; Auto Register Duplication                                                  ; Auto                           ; Auto                           ;
; Auto Global Clock                                                          ; On                             ; On                             ;
; Auto Global Register Control Signals                                       ; On                             ; On                             ;
; Stop After Congestion Map Generation                                       ; Off                            ; Off                            ;
; Save Intermediate Fitting Results                                          ; Off                            ; Off                            ;
; Force Fitter to Avoid Periphery Placement Warnings                         ; Off                            ; Off                            ;
; Use Best Effort Settings for Compilation                                   ; Off                            ; Off                            ;
+----------------------------------------------------------------------------+--------------------------------+--------------------------------+


+------------------------------------------+
; Parallel Compilation                     ;
+----------------------------+-------------+
; Processors                 ; Number      ;
+----------------------------+-------------+
; Number detected on machine ; 2           ;
; Maximum allowed            ; 2           ;
;                            ;             ;
; Average used               ; 1.47        ;
; Maximum used               ; 2           ;
;                            ;             ;
; Usage by Processor         ; % Time Used ;
;     1 processor            ; 100.0%      ;
;     2 processors           ;  30.4%      ;
+----------------------------+-------------+


+--------------+
; Pin-Out File ;
+--------------+
The pin-out file can be found in D:/synchro_portable/Data/ASIC/skiroc2/firmware/Skiroc2.pin.


+---------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Usage Summary                                                                                                   ;
+---------------------------------------------+-----------------------------------------------------------------------------------+
; Resource                                    ; Usage                                                                             ;
+---------------------------------------------+-----------------------------------------------------------------------------------+
; Total logic elements                        ; 2,431 / 5,980 ( 41 % )                                                            ;
;     -- Combinational with no register       ; 683                                                                               ;
;     -- Register only                        ; 673                                                                               ;
;     -- Combinational with a register        ; 1075                                                                              ;
;                                             ;                                                                                   ;
; Logic element usage by number of LUT inputs ;                                                                                   ;
;     -- 4 input functions                    ; 869                                                                               ;
;     -- 3 input functions                    ; 577                                                                               ;
;     -- 2 input functions                    ; 278                                                                               ;
;     -- 1 input functions                    ; 22                                                                                ;
;     -- 0 input functions                    ; 12                                                                                ;
;                                             ;                                                                                   ;
; Logic elements by mode                      ;                                                                                   ;
;     -- normal mode                          ; 2056                                                                              ;
;     -- arithmetic mode                      ; 375                                                                               ;
;     -- qfbk mode                            ; 285                                                                               ;
;     -- register cascade mode                ; 0                                                                                 ;
;     -- synchronous clear/load mode          ; 766                                                                               ;
;     -- asynchronous clear/load mode         ; 1734                                                                              ;
;                                             ;                                                                                   ;
; Total registers                             ; 1,748 / 6,523 ( 27 % )                                                            ;
; Total LABs                                  ; 287 / 598 ( 48 % )                                                                ;
; Logic elements in carry chains              ; 416                                                                               ;
; User inserted logic elements                ; 0                                                                                 ;
; Virtual pins                                ; 0                                                                                 ;
; I/O pins                                    ; 141 / 185 ( 76 % )                                                                ;
;     -- Clock pins                           ; 1 / 2 ( 50 % )                                                                    ;
; Global signals                              ; 8                                                                                 ;
; M4Ks                                        ; 17 / 20 ( 85 % )                                                                  ;
; Total memory bits                           ; 67,584 / 92,160 ( 73 % )                                                          ;
; Total RAM block bits                        ; 78,336 / 92,160 ( 85 % )                                                          ;
; PLLs                                        ; 1 / 2 ( 50 % )                                                                    ;
; Global clocks                               ; 8 / 8 ( 100 % )                                                                   ;
; JTAGs                                       ; 0 / 1 ( 0 % )                                                                     ;
; ASMI Blocks                                 ; 0 / 1 ( 0 % )                                                                     ;
; CRC blocks                                  ; 0 / 1 ( 0 % )                                                                     ;
; Average interconnect usage (total/H/V)      ; 18% / 19% / 17%                                                                   ;
; Peak interconnect usage (total/H/V)         ; 43% / 46% / 40%                                                                   ;
; Maximum fan-out node                        ; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[2] ;
; Maximum fan-out                             ; 677                                                                               ;
; Highest non-global fan-out signal           ; pwr_reset                                                                         ;
; Highest non-global fan-out                  ; 465                                                                               ;
; Total fan-out                               ; 10948                                                                             ;
; Average fan-out                             ; 4.22                                                                              ;
+---------------------------------------------+-----------------------------------------------------------------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Input Pins                                                                                                                                                                                                                                                           ;
+----------------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+-------------+----------------------+
; Name           ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Cell number ; Combinational Fan-Out ; Registered Fan-Out ; Global ; Input Register ; Power Up High ; PCI I/O Enabled ; Bus Hold ; Weak Pull Up ; I/O Standard ; Termination ; Location assigned by ;
+----------------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+-------------+----------------------+
; ADC[0]         ; 138   ; 3        ; 35           ; 7            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[10]        ; 126   ; 3        ; 35           ; 3            ; 2           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[11]        ; 125   ; 3        ; 35           ; 2            ; 0           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[1]         ; 137   ; 3        ; 35           ; 6            ; 0           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[2]         ; 136   ; 3        ; 35           ; 6            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[3]         ; 135   ; 3        ; 35           ; 5            ; 0           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[4]         ; 134   ; 3        ; 35           ; 5            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[5]         ; 133   ; 3        ; 35           ; 4            ; 0           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[6]         ; 132   ; 3        ; 35           ; 4            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[7]         ; 131   ; 3        ; 35           ; 4            ; 2           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[8]         ; 128   ; 3        ; 35           ; 3            ; 0           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ADC[9]         ; 127   ; 3        ; 35           ; 3            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; ChipSatb       ; 115   ; 4        ; 32           ; 0            ; 2           ; 4                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; Dout1b         ; 118   ; 4        ; 34           ; 0            ; 2           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; Dout2b         ; 119   ; 4        ; 34           ; 0            ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; IN_ALTERA1     ; 234   ; 2        ; 6            ; 21           ; 2           ; 3                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; IN_ALTERA2     ; 228   ; 2        ; 6            ; 21           ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; IN_ALTERA3     ; 226   ; 2        ; 8            ; 21           ; 1           ; 4                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; IN_ALTERA4     ; 224   ; 2        ; 10           ; 21           ; 2           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; IN_ALTERA5     ; 222   ; 2        ; 10           ; 21           ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; IN_ALTERA6     ; 220   ; 2        ; 12           ; 21           ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; OTR            ; 124   ; 3        ; 35           ; 2            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; TransmitOn1b   ; 116   ; 4        ; 32           ; 0            ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; TransmitOn2b   ; 117   ; 4        ; 32           ; 0            ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; TrigOutb       ; 120   ; 4        ; 34           ; 0            ; 0           ; 4                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; XTIN           ; 177   ; 3        ; 35           ; 19           ; 1           ; 0                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; clk_gene_ext   ; 238   ; 2        ; 2            ; 21           ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; clk_osc        ; 28    ; 1        ; 0            ; 12           ; 2           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; digital_probe1 ; 73    ; 4        ; 6            ; 0            ; 0           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; digital_probe2 ; 74    ; 4        ; 8            ; 0            ; 2           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; end_readout1   ; 75    ; 4        ; 8            ; 0            ; 1           ; 6                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; end_readout2   ; 76    ; 4        ; 8            ; 0            ; 0           ; 5                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; hold_conn      ; 236   ; 2        ; 4            ; 21           ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 1.5 V        ; Off         ; User                 ;
; nRXF           ; 163   ; 3        ; 35           ; 15           ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; nTXE           ; 164   ; 3        ; 35           ; 15           ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 2.5 V        ; Off         ; User                 ;
; pwr_reset      ; 121   ; 3        ; 35           ; 1            ; 1           ; 464                   ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; sr_out         ; 68    ; 4        ; 6            ; 0            ; 1           ; 2                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; srout_read     ; 67    ; 4        ; 6            ; 0            ; 2           ; 3                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
+----------------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+-------------+----------------------+


+---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Output Pins                                                                                                                                                                                                                                                                                                                                                         ;
+---------------------+-------+----------+--------------+--------------+-------------+-----------------+------------------------+---------------+----------------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-------------+----------------------+-------+----------------------+---------------------+
; Name                ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Cell number ; Output Register ; Output Enable Register ; Power Up High ; Slow Slew Rate ; PCI I/O Enabled ; Open Drain ; TRI Primitive ; Bus Hold ; Weak Pull Up ; I/O Standard ; Current Strength ; Termination ; Location assigned by ; Load  ; Output Enable Source ; Output Enable Group ;
+---------------------+-------+----------+--------------+--------------+-------------+-----------------+------------------------+---------------+----------------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-------------+----------------------+-------+----------------------+---------------------+
; 40M                 ; 86    ; 4        ; 16           ; 0            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; 40M(n)              ; 87    ; 4        ; 16           ; 0            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; 40M_test            ; 58    ; 1        ; 0            ; 2            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; 5M                  ; 82    ; 4        ; 12           ; 0            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; 5M(n)               ; 83    ; 4        ; 14           ; 0            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; LED                 ; 61    ; 4        ; 2            ; 0            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; PLL_OUT             ; 38    ; 1        ; 0            ; 8            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; R_C                 ; 104   ; 4        ; 26           ; 0            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; R_C(n)              ; 105   ; 4        ; 28           ; 0            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; SYNC_GENE           ; 2     ; 1        ; 0            ; 20           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; T_E                 ; 100   ; 4        ; 24           ; 0            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; T_E(n)              ; 101   ; 4        ; 24           ; 0            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; V_E                 ; 96    ; 4        ; 22           ; 0            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; V_E(n)              ; 97    ; 4        ; 22           ; 0            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; LVDS         ; Maximum Current  ; Off         ; User                 ; 4 pF  ; -                    ; -                   ;
; WR                  ; 165   ; 3        ; 35           ; 16           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; adc_clk             ; 1     ; 1        ; 0            ; 20           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; ck_read             ; 42    ; 1        ; 0            ; 7            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; yes           ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; hold                ; 240   ; 2        ; 2            ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; nRD                 ; 166   ; 3        ; 35           ; 16           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; out_altera1         ; 144   ; 3        ; 35           ; 9            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; out_altera2         ; 156   ; 3        ; 35           ; 13           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; out_altera3         ; 158   ; 3        ; 35           ; 13           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; out_altera4         ; 159   ; 3        ; 35           ; 13           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; out_altera5         ; 160   ; 3        ; 35           ; 14           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; out_altera6         ; 161   ; 3        ; 35           ; 14           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; pwr_on_a            ; 44    ; 1        ; 0            ; 6            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; pwr_on_adc          ; 45    ; 1        ; 0            ; 6            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; pwr_on_d            ; 47    ; 1        ; 0            ; 5            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; pwr_on_dac          ; 46    ; 1        ; 0            ; 5            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; resetb              ; 54    ; 1        ; 0            ; 3            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; rstb_pa             ; 41    ; 1        ; 0            ; 7            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; select              ; 53    ; 1        ; 0            ; 3            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; sr_ck               ; 50    ; 1        ; 0            ; 4            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; yes           ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; sr_in               ; 48    ; 1        ; 0            ; 4            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; yes           ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; sr_rstb             ; 49    ; 1        ; 0            ; 4            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; srin_read           ; 43    ; 1        ; 0            ; 7            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; yes           ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; start_acq           ; 21    ; 1        ; 0            ; 14           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; start_convb         ; 57    ; 1        ; 0            ; 2            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; start_ramp_tdc_ext  ; 60    ; 1        ; 0            ; 1            ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; start_rampb_adc_ext ; 59    ; 1        ; 0            ; 1            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; start_readout1      ; 55    ; 1        ; 0            ; 3            ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; start_readout2      ; 56    ; 1        ; 0            ; 2            ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test1               ; 239   ; 2        ; 2            ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test10              ; 218   ; 2        ; 14           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test11              ; 217   ; 2        ; 14           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test12              ; 216   ; 2        ; 14           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test13              ; 215   ; 2        ; 16           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test14              ; 214   ; 2        ; 16           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test15              ; 213   ; 2        ; 16           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test16              ; 207   ; 2        ; 20           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test17              ; 206   ; 2        ; 20           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test18              ; 205   ; 2        ; 22           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test19              ; 204   ; 2        ; 22           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test2               ; 237   ; 2        ; 4            ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test20              ; 203   ; 2        ; 22           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test21              ; 202   ; 2        ; 24           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test22              ; 201   ; 2        ; 24           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test23              ; 200   ; 2        ; 24           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test24              ; 199   ; 2        ; 26           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test25              ; 198   ; 2        ; 26           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test26              ; 197   ; 2        ; 26           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test27              ; 196   ; 2        ; 28           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test28              ; 195   ; 2        ; 28           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test29              ; 194   ; 2        ; 28           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test3               ; 235   ; 2        ; 4            ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test30              ; 193   ; 2        ; 30           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test31              ; 188   ; 2        ; 30           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test32              ; 187   ; 2        ; 30           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test33              ; 186   ; 2        ; 32           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test34              ; 185   ; 2        ; 32           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test35              ; 184   ; 2        ; 32           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test36              ; 183   ; 2        ; 34           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test37              ; 182   ; 2        ; 34           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test38              ; 181   ; 2        ; 34           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test39              ; 180   ; 3        ; 35           ; 20           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test4               ; 233   ; 2        ; 6            ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test40              ; 179   ; 3        ; 35           ; 20           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test5               ; 227   ; 2        ; 8            ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test6               ; 225   ; 2        ; 8            ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test7               ; 223   ; 2        ; 10           ; 21           ; 1           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test8               ; 221   ; 2        ; 12           ; 21           ; 2           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
; test9               ; 219   ; 2        ; 12           ; 21           ; 0           ; no              ; no                     ; no            ; no             ; no              ; no         ; no            ; no       ; Off          ; 1.5 V        ; 8mA              ; Off         ; User                 ; 10 pF ; -                    ; -                   ;
+---------------------+-------+----------+--------------+--------------+-------------+-----------------+------------------------+---------------+----------------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-------------+----------------------+-------+----------------------+---------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Bidir Pins                                                                                                                                                                                                                                                                                                                                                                                                                     ;
+--------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+-----------------+------------------------+---------------+----------------+-----------------+------------+----------+--------------+--------------+------------------+-------------+----------------------+-------+---------------------------------------+---------------------+
; Name   ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Cell number ; Combinational Fan-Out ; Registered Fan-Out ; Global ; Input Register ; Output Register ; Output Enable Register ; Power Up High ; Slow Slew Rate ; PCI I/O Enabled ; Open Drain ; Bus Hold ; Weak Pull Up ; I/O Standard ; Current Strength ; Termination ; Location assigned by ; Load  ; Output Enable Source                  ; Output Enable Group ;
+--------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+-----------------+------------------------+---------------+----------------+-----------------+------------+----------+--------------+--------------+------------------+-------------+----------------------+-------+---------------------------------------+---------------------+
; DAQ0   ; 19    ; 1        ; 0            ; 14           ; 0           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ1   ; 17    ; 1        ; 0            ; 15           ; 0           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ10  ; 8     ; 1        ; 0            ; 18           ; 2           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ11  ; 5     ; 1        ; 0            ; 19           ; 2           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ12  ; 6     ; 1        ; 0            ; 18           ; 0           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ2   ; 18    ; 1        ; 0            ; 15           ; 1           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ3   ; 15    ; 1        ; 0            ; 16           ; 1           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ4   ; 16    ; 1        ; 0            ; 16           ; 2           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ5   ; 13    ; 1        ; 0            ; 17           ; 2           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ6   ; 14    ; 1        ; 0            ; 16           ; 0           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ7   ; 11    ; 1        ; 0            ; 17           ; 0           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ8   ; 12    ; 1        ; 0            ; 17           ; 1           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; DAQ9   ; 7     ; 1        ; 0            ; 18           ; 1           ; 0                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 10 pF ; -                                     ; -                   ;
; USB[0] ; 176   ; 3        ; 35           ; 19           ; 2           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[1] ; 173   ; 3        ; 35           ; 18           ; 2           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[2] ; 174   ; 3        ; 35           ; 18           ; 1           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[3] ; 167   ; 3        ; 35           ; 16           ; 0           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[4] ; 175   ; 3        ; 35           ; 18           ; 0           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[5] ; 169   ; 3        ; 35           ; 17           ; 1           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[6] ; 168   ; 3        ; 35           ; 17           ; 2           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
; USB[7] ; 170   ; 3        ; 35           ; 17           ; 0           ; 1                     ; 0                  ; no     ; no             ; no              ; no                     ; no            ; no             ; no              ; no         ; no       ; Off          ; 2.5 V        ; 16mA             ; Off         ; User                 ; 10 pF ; usb_full_interface_v:inst10|always2~1 ; -                   ;
+--------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+-----------------+------------------------+---------------+----------------+-----------------+------------+----------+--------------+--------------+------------------+-------------+----------------------+-------+---------------------------------------+---------------------+


+------------------------------------------------------------+
; I/O Bank Usage                                             ;
+----------+------------------+---------------+--------------+
; I/O Bank ; Usage            ; VCCIO Voltage ; VREF Voltage ;
+----------+------------------+---------------+--------------+
; 1        ; 38 / 44 ( 86 % ) ; 3.3V          ; --           ;
; 2        ; 47 / 48 ( 98 % ) ; 1.5V          ; --           ;
; 3        ; 35 / 45 ( 78 % ) ; 2.5V          ; --           ;
; 4        ; 23 / 48 ( 48 % ) ; 2.5V          ; --           ;
+----------+------------------+---------------+--------------+


+-------------------------------------------------------------------------------------------------------------------------------------------------------+
; All Package Pins                                                                                                                                      ;
+----------+------------+----------+-------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
; Location ; Pad Number ; I/O Bank ; Pin Name/Usage          ; Dir.   ; I/O Standard ; Voltage ; I/O Type   ; User Assignment ; Bus Hold ; Weak Pull Up ;
+----------+------------+----------+-------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
; 1        ; 0          ; 1        ; adc_clk                 ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 2        ; 1          ; 1        ; SYNC_GENE               ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 3        ; 2          ; 1        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 4        ; 3          ; 1        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 5        ; 4          ; 1        ; DAQ11                   ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 6        ; 5          ; 1        ; DAQ12                   ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 7        ; 6          ; 1        ; DAQ9                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 8        ; 7          ; 1        ; DAQ10                   ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 9        ;            ; 1        ; VCCIO1                  ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; 10       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 11       ; 8          ; 1        ; DAQ7                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 12       ; 9          ; 1        ; DAQ8                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 13       ; 10         ; 1        ; DAQ5                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 14       ; 11         ; 1        ; DAQ6                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 15       ; 12         ; 1        ; DAQ3                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 16       ; 13         ; 1        ; DAQ4                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 17       ; 14         ; 1        ; DAQ1                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 18       ; 15         ; 1        ; DAQ2                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 19       ; 16         ; 1        ; DAQ0                    ; bidir  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 20       ; 17         ; 1        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 21       ; 18         ; 1        ; start_acq               ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 22       ;            ; 1        ; VCCIO1                  ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; 23       ; 19         ; 1        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 24       ; 20         ; 1        ; ~nCSO~ / RESERVED_INPUT ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; N               ; no       ; Off          ;
; 25       ; 21         ; 1        ; ^DATA0                  ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; 26       ; 22         ; 1        ; ^nCONFIG                ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 27       ;            ;          ; VCCA_PLL1               ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 28       ; 23         ; 1        ; clk_osc                 ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 29       ; 24         ; 1        ; GND+                    ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; 30       ;            ;          ; GNDA_PLL1               ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 31       ;            ;          ; GNDG_PLL1               ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 32       ; 25         ; 1        ; ^nCEO                   ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 33       ; 26         ; 1        ; ^nCE                    ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 34       ; 27         ; 1        ; ^MSEL0                  ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 35       ; 28         ; 1        ; ^MSEL1                  ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 36       ; 29         ; 1        ; ^DCLK                   ; bidir  ;              ;         ; --         ;                 ; --       ; --           ;
; 37       ; 30         ; 1        ; ~ASDO~ / RESERVED_INPUT ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; N               ; no       ; Off          ;
; 38       ; 31         ; 1        ; PLL_OUT                 ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 39       ; 32         ; 1        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 40       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 41       ; 33         ; 1        ; rstb_pa                 ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 42       ; 34         ; 1        ; ck_read                 ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 43       ; 35         ; 1        ; srin_read               ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 44       ; 36         ; 1        ; pwr_on_a                ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 45       ; 37         ; 1        ; pwr_on_adc              ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 46       ; 38         ; 1        ; pwr_on_dac              ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 47       ; 39         ; 1        ; pwr_on_d                ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 48       ; 40         ; 1        ; sr_in                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 49       ; 41         ; 1        ; sr_rstb                 ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 50       ; 42         ; 1        ; sr_ck                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 51       ;            ; 1        ; VCCIO1                  ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; 52       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 53       ; 43         ; 1        ; select                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 54       ; 44         ; 1        ; resetb                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 55       ; 45         ; 1        ; start_readout1          ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 56       ; 46         ; 1        ; start_readout2          ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 57       ; 47         ; 1        ; start_convb             ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 58       ; 48         ; 1        ; 40M_test                ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 59       ; 49         ; 1        ; start_rampb_adc_ext     ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 60       ; 50         ; 1        ; start_ramp_tdc_ext      ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 61       ; 51         ; 4        ; LED                     ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 62       ; 52         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 63       ; 53         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 64       ; 54         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 65       ; 55         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 66       ; 56         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 67       ; 57         ; 4        ; srout_read              ; input  ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; 68       ; 58         ; 4        ; sr_out                  ; input  ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; 69       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 70       ;            ; 4        ; VCCIO4                  ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; 71       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 72       ;            ;          ; VCCINT                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 73       ; 59         ; 4        ; digital_probe1          ; input  ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; 74       ; 60         ; 4        ; digital_probe2          ; input  ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; 75       ; 61         ; 4        ; end_readout1            ; input  ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; 76       ; 62         ; 4        ; end_readout2            ; input  ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; 77       ; 63         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 78       ; 64         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 79       ; 65         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 80       ; 66         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 81       ; 67         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 82       ; 68         ; 4        ; 5M                      ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 83       ; 69         ; 4        ; 5M(n)                   ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 84       ; 70         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 85       ; 71         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 86       ; 72         ; 4        ; 40M                     ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 87       ; 73         ; 4        ; 40M(n)                  ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 88       ; 74         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 89       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 90       ;            ;          ; VCCINT                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 91       ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 92       ;            ; 4        ; VCCIO4                  ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; 93       ; 75         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 94       ; 76         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 95       ; 77         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 96       ; 78         ; 4        ; V_E                     ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 97       ; 79         ; 4        ; V_E(n)                  ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 98       ; 80         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 99       ; 81         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 100      ; 82         ; 4        ; T_E                     ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 101      ; 83         ; 4        ; T_E(n)                  ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 102      ; 84         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 103      ; 85         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 104      ; 86         ; 4        ; R_C                     ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 105      ; 87         ; 4        ; R_C(n)                  ; output ; LVDS         ;         ; Column I/O ; Y               ; no       ; Off          ;
; 106      ; 88         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 107      ; 89         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 108      ; 90         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 109      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 110      ;            ;          ; VCCINT                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 111      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 112      ;            ; 4        ; VCCIO4                  ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; 113      ; 91         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 114      ; 92         ; 4        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 115      ; 93         ; 4        ; ChipSatb                ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 116      ; 94         ; 4        ; TransmitOn1b            ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 117      ; 95         ; 4        ; TransmitOn2b            ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 118      ; 96         ; 4        ; Dout1b                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 119      ; 97         ; 4        ; Dout2b                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 120      ; 98         ; 4        ; TrigOutb                ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 121      ; 99         ; 3        ; pwr_reset               ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 122      ; 100        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 123      ; 101        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 124      ; 102        ; 3        ; OTR                     ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 125      ; 103        ; 3        ; ADC[11]                 ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 126      ; 104        ; 3        ; ADC[10]                 ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 127      ; 105        ; 3        ; ADC[9]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 128      ; 106        ; 3        ; ADC[8]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 129      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 130      ;            ; 3        ; VCCIO3                  ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; 131      ; 107        ; 3        ; ADC[7]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 132      ; 108        ; 3        ; ADC[6]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 133      ; 109        ; 3        ; ADC[5]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 134      ; 110        ; 3        ; ADC[4]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 135      ; 111        ; 3        ; ADC[3]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 136      ; 112        ; 3        ; ADC[2]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 137      ; 113        ; 3        ; ADC[1]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 138      ; 114        ; 3        ; ADC[0]                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 139      ; 115        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 140      ; 116        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 141      ; 117        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 142      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 143      ; 118        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 144      ; 119        ; 3        ; out_altera1             ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 145      ; 120        ; 3        ; ^CONF_DONE              ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 146      ; 121        ; 3        ; ^nSTATUS                ;        ;              ;         ; --         ;                 ; --       ; --           ;
; 147      ; 122        ; 3        ; #TCK                    ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; 148      ; 123        ; 3        ; #TMS                    ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; 149      ; 124        ; 3        ; #TDO                    ; output ;              ;         ; --         ;                 ; --       ; --           ;
; 150      ;            ;          ; GNDG_PLL2               ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 151      ;            ;          ; GNDA_PLL2               ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 152      ; 125        ; 3        ; GND+                    ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; 153      ; 126        ; 3        ; GND+                    ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; 154      ;            ;          ; VCCA_PLL2               ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 155      ; 127        ; 3        ; #TDI                    ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; 156      ; 128        ; 3        ; out_altera2             ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 157      ;            ; 3        ; VCCIO3                  ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; 158      ; 129        ; 3        ; out_altera3             ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 159      ; 130        ; 3        ; out_altera4             ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 160      ; 131        ; 3        ; out_altera5             ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 161      ; 132        ; 3        ; out_altera6             ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 162      ; 133        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 163      ; 134        ; 3        ; nRXF                    ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 164      ; 135        ; 3        ; nTXE                    ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 165      ; 136        ; 3        ; WR                      ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 166      ; 137        ; 3        ; nRD                     ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 167      ; 138        ; 3        ; USB[3]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 168      ; 139        ; 3        ; USB[6]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 169      ; 140        ; 3        ; USB[5]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 170      ; 141        ; 3        ; USB[7]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 171      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 172      ;            ; 3        ; VCCIO3                  ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; 173      ; 142        ; 3        ; USB[1]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 174      ; 143        ; 3        ; USB[2]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 175      ; 144        ; 3        ; USB[4]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 176      ; 145        ; 3        ; USB[0]                  ; bidir  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 177      ; 146        ; 3        ; XTIN                    ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 178      ; 147        ; 3        ; RESERVED_INPUT          ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; 179      ; 148        ; 3        ; test40                  ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 180      ; 149        ; 3        ; test39                  ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; 181      ; 150        ; 2        ; test38                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 182      ; 151        ; 2        ; test37                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 183      ; 152        ; 2        ; test36                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 184      ; 153        ; 2        ; test35                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 185      ; 154        ; 2        ; test34                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 186      ; 155        ; 2        ; test33                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 187      ; 156        ; 2        ; test32                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 188      ; 157        ; 2        ; test31                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 189      ;            ; 2        ; VCCIO2                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 190      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 191      ;            ;          ; VCCINT                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 192      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 193      ; 158        ; 2        ; test30                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 194      ; 159        ; 2        ; test29                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 195      ; 160        ; 2        ; test28                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 196      ; 161        ; 2        ; test27                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 197      ; 162        ; 2        ; test26                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 198      ; 163        ; 2        ; test25                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 199      ; 164        ; 2        ; test24                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 200      ; 165        ; 2        ; test23                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 201      ; 166        ; 2        ; test22                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 202      ; 167        ; 2        ; test21                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 203      ; 168        ; 2        ; test20                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 204      ; 169        ; 2        ; test19                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 205      ; 170        ; 2        ; test18                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 206      ; 171        ; 2        ; test17                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 207      ; 172        ; 2        ; test16                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 208      ; 173        ; 2        ; RESERVED_INPUT          ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; 209      ;            ; 2        ; VCCIO2                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 210      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 211      ;            ;          ; VCCINT                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 212      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 213      ; 174        ; 2        ; test15                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 214      ; 175        ; 2        ; test14                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 215      ; 176        ; 2        ; test13                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 216      ; 177        ; 2        ; test12                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 217      ; 178        ; 2        ; test11                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 218      ; 179        ; 2        ; test10                  ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 219      ; 180        ; 2        ; test9                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 220      ; 181        ; 2        ; IN_ALTERA6              ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 221      ; 182        ; 2        ; test8                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 222      ; 183        ; 2        ; IN_ALTERA5              ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 223      ; 184        ; 2        ; test7                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 224      ; 185        ; 2        ; IN_ALTERA4              ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 225      ; 186        ; 2        ; test6                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 226      ; 187        ; 2        ; IN_ALTERA3              ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 227      ; 188        ; 2        ; test5                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 228      ; 189        ; 2        ; IN_ALTERA2              ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 229      ;            ;          ; VCCINT                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 230      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 231      ;            ; 2        ; VCCIO2                  ; power  ;              ; 1.5V    ; --         ;                 ; --       ; --           ;
; 232      ;            ;          ; GND                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; 233      ; 190        ; 2        ; test4                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 234      ; 191        ; 2        ; IN_ALTERA1              ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 235      ; 192        ; 2        ; test3                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 236      ; 193        ; 2        ; hold_conn               ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 237      ; 194        ; 2        ; test2                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 238      ; 195        ; 2        ; clk_gene_ext            ; input  ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 239      ; 196        ; 2        ; test1                   ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; 240      ; 197        ; 2        ; hold                    ; output ; 1.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
+----------+------------+----------+-------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
Note: Pin directions (input, output or bidir) are based on device operating in user mode.


+--------------------------------------------------------------------------+
; PLL Summary                                                              ;
+-------------------------------+------------------------------------------+
; Name                          ; pll_sk2:inst|altpll:altpll_component|pll ;
+-------------------------------+------------------------------------------+
; SDC pin name                  ; inst|altpll_component|pll                ;
; PLL type                      ; -                                        ;
; Scan chain                    ; None                                     ;
; PLL mode                      ; Normal                                   ;
; Feedback source               ; --                                       ;
; Compensate clock              ; clock0                                   ;
; Compensated input/output pins ; --                                       ;
; Switchover on loss of clock   ; --                                       ;
; Switchover counter            ; --                                       ;
; Primary clock                 ; --                                       ;
; Input frequency 0             ; 40.0 MHz                                 ;
; Input frequency 1             ; --                                       ;
; Nominal PFD frequency         ; 40.0 MHz                                 ;
; Nominal VCO frequency         ; 800.0 MHz                                ;
; Freq min lock                 ; 24.55 MHz                                ;
; Freq max lock                 ; 50.0 MHz                                 ;
; Clock Offset                  ; 0 ps                                     ;
; M VCO Tap                     ; 0                                        ;
; M Initial                     ; 1                                        ;
; M value                       ; 20                                       ;
; N value                       ; 1                                        ;
; M counter delay               ; --                                       ;
; N counter delay               ; --                                       ;
; M2 value                      ; --                                       ;
; N2 value                      ; --                                       ;
; SS counter                    ; --                                       ;
; Downspread                    ; --                                       ;
; Spread frequency              ; --                                       ;
; enable0 counter               ; --                                       ;
; enable1 counter               ; --                                       ;
; Real time reconfigurable      ; --                                       ;
; Scan chain MIF file           ; --                                       ;
; Preserve PLL counter order    ; Off                                      ;
; PLL location                  ; PLL_1                                    ;
; Inclk0 signal                 ; clk_osc                                  ;
; Inclk1 signal                 ; --                                       ;
; Inclk0 signal type            ; Dedicated Pin                            ;
; Inclk1 signal type            ; --                                       ;
+-------------------------------+------------------------------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; PLL Usage                                                                                                                                                                                                                                  ;
+--------------------------------------------+--------------+------+-----+------------------+-------------+-------+------------+---------+---------------+---------------+------------+---------+---------+----------------------------------+
; Name                                       ; Output Clock ; Mult ; Div ; Output Frequency ; Phase Shift ; Delay ; Duty Cycle ; Counter ; Counter Delay ; Counter Value ; High / Low ; Initial ; VCO Tap ; SDC Pin Name                     ;
+--------------------------------------------+--------------+------+-----+------------------+-------------+-------+------------+---------+---------------+---------------+------------+---------+---------+----------------------------------+
; pll_sk2:inst|altpll:altpll_component|_clk0 ; clock0       ; 4    ; 1   ; 160.0 MHz        ; 0 (0 ps)    ; 0 ps  ; 50/50      ; G0      ; --            ; 5             ; 3/2 Odd    ; 1       ; 0       ; inst|altpll_component|pll|clk[0] ;
; pll_sk2:inst|altpll:altpll_component|_clk1 ; clock1       ; 10   ; 1   ; 400.0 MHz        ; 0 (0 ps)    ; 0 ps  ; 50/50      ; G1      ; --            ; 2             ; 1/1 Even   ; 1       ; 0       ; inst|altpll_component|pll|clk[1] ;
+--------------------------------------------+--------------+------+-----+------------------+-------------+-------+------------+---------+---------------+---------------+------------+---------+---------+----------------------------------+


+------------------------------------------------------------------+
; Output Pin Default Load For Reported TCO                         ;
+---------------------+-------+------------------------------------+
; I/O Standard        ; Load  ; Termination Resistance             ;
+---------------------+-------+------------------------------------+
; 3.3-V LVTTL         ; 10 pF ; Not Available                      ;
; 3.3-V LVCMOS        ; 10 pF ; Not Available                      ;
; 2.5 V               ; 10 pF ; Not Available                      ;
; 1.8 V               ; 10 pF ; Not Available                      ;
; 1.5 V               ; 10 pF ; Not Available                      ;
; SSTL-3 Class I      ; 30 pF ; 50 Ohm (Parallel), 25 Ohm (Serial) ;
; SSTL-3 Class II     ; 30 pF ; 25 Ohm (Parallel), 25 Ohm (Serial) ;
; SSTL-2 Class I      ; 30 pF ; 50 Ohm (Parallel), 25 Ohm (Serial) ;
; SSTL-2 Class II     ; 30 pF ; 25 Ohm (Parallel), 25 Ohm (Serial) ;
; Differential SSTL-2 ; 10 pF ; (See SSTL-2)                       ;
; 3.3-V PCI           ; 10 pF ; 25 Ohm (Parallel)                  ;
; LVDS                ; 4 pF  ; 100 Ohm (Differential)             ;
; RSDS                ; 10 pF ; 100 Ohm (Differential)             ;
+---------------------+-------+------------------------------------+
Note: User assignments will override these defaults. The user specified values are listed in the Output Pins and Bidir Pins tables.


+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Utilization by Entity                                                                                                                                                                                                                                                                                                                                                                             ;
+-----------------------------------------------------+-------------+--------------+-------------+------+------+--------------+--------------+-------------------+------------------+-----------------+------------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+--------------+
; Compilation Hierarchy Node                          ; Logic Cells ; LC Registers ; Memory Bits ; M4Ks ; Pins ; Virtual Pins ; LUT-Only LCs ; Register-Only LCs ; LUT/Register LCs ; Carry Chain LCs ; Packed LCs ; Full Hierarchy Name                                                                                                                                                             ; Library Name ;
+-----------------------------------------------------+-------------+--------------+-------------+------+------+--------------+--------------+-------------------+------------------+-----------------+------------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+--------------+
; |Skiroc2                                            ; 2431 (31)   ; 1748         ; 67584       ; 17   ; 141  ; 0            ; 683 (27)     ; 673 (1)           ; 1075 (3)         ; 416 (0)         ; 274 (5)    ; |Skiroc2                                                                                                                                                                        ; work         ;
;    |ADC_AD9220_all:inst200|                         ; 433 (43)    ; 353          ; 16384       ; 4    ; 0    ; 0            ; 80 (36)      ; 145 (0)           ; 208 (7)          ; 100 (0)         ; 11 (1)     ; |Skiroc2|ADC_AD9220_all:inst200                                                                                                                                                 ; work         ;
;       |Read_Word:Read_Word22|                       ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|Read_Word:Read_Word22                                                                                                                           ; work         ;
;       |Read_Word:Read_Word24|                       ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|Read_Word:Read_Word24                                                                                                                           ; work         ;
;       |counter_10b:counter_10b_evt|                 ; 10 (0)      ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (0)           ; 10 (0)          ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|counter_10b:counter_10b_evt                                                                                                                     ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 10 (0)      ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (0)           ; 10 (0)          ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|counter_10b:counter_10b_evt|lpm_counter:lpm_counter_component                                                                                   ; work         ;
;             |cntr_chi:auto_generated|               ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|counter_10b:counter_10b_evt|lpm_counter:lpm_counter_component|cntr_chi:auto_generated                                                           ; work         ;
;       |counter_10b:counter_10b_inst|                ; 10 (0)      ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (0)           ; 10 (0)          ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|counter_10b:counter_10b_inst                                                                                                                    ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 10 (0)      ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (0)           ; 10 (0)          ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|counter_10b:counter_10b_inst|lpm_counter:lpm_counter_component                                                                                  ; work         ;
;             |cntr_chi:auto_generated|               ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|counter_10b:counter_10b_inst|lpm_counter:lpm_counter_component|cntr_chi:auto_generated                                                          ; work         ;
;       |fifo_adc:fifo_adc_inst_20|                   ; 185 (0)     ; 163          ; 8192        ; 2    ; 0    ; 0            ; 22 (0)       ; 72 (0)            ; 91 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20                                                                                                                       ; work         ;
;          |dcfifo:dcfifo_component|                  ; 185 (0)     ; 163          ; 8192        ; 2    ; 0    ; 0            ; 22 (0)       ; 72 (0)            ; 91 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component                                                                                               ; work         ;
;             |dcfifo_pdi1:auto_generated|            ; 185 (12)    ; 163          ; 8192        ; 2    ; 0    ; 0            ; 22 (2)       ; 72 (10)           ; 91 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated                                                                    ; work         ;
;                |a_fefifo_30d:read_state|            ; 12 (12)     ; 4            ; 0           ; 0    ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 4 (4)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_fefifo_30d:read_state                                            ; work         ;
;                |a_fefifo_pdc:write_state|           ; 3 (3)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_fefifo_pdc:write_state                                           ; work         ;
;                |a_gray2bin_26b:gray2bin_rs_nbwp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_gray2bin_26b:gray2bin_rs_nbwp                                    ; work         ;
;                |a_gray2bin_26b:gray2bin_ws_nbrp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_gray2bin_26b:gray2bin_ws_nbrp                                    ; work         ;
;                |a_graycounter_626:rdptr_g|          ; 20 (20)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_graycounter_626:rdptr_g                                          ; work         ;
;                |a_graycounter_626:wrptr_g|          ; 18 (18)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 4 (4)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_graycounter_626:wrptr_g                                          ; work         ;
;                |alt_synch_pipe_0e8:dffpipe_rs_dgwp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_rs_dgwp                                 ; work         ;
;                   |dffpipe_qe9:dffpipe9|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_rs_dgwp|dffpipe_qe9:dffpipe9            ; work         ;
;                |alt_synch_pipe_0e8:dffpipe_ws_dgrp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp                                 ; work         ;
;                   |dffpipe_qe9:dffpipe9|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp|dffpipe_qe9:dffpipe9            ; work         ;
;                |cntr_kua:rdptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|cntr_kua:rdptr_b                                                   ; work         ;
;                |cntr_kua:wrptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|cntr_kua:wrptr_b                                                   ; work         ;
;                |dffpipe_oe9:dffpipe_rdbuw|          ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_rdbuw                                          ; work         ;
;                |dffpipe_oe9:dffpipe_rs_dbwp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_rs_dbwp                                        ; work         ;
;                |dffpipe_oe9:dffpipe_wr_dbuw|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_wr_dbuw                                        ; work         ;
;                |dffpipe_oe9:dffpipe_ws_nbrp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_ws_nbrp                                        ; work         ;
;                |dpram_n3v:fiforam|                  ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam                                                  ; work         ;
;                   |altsyncram_pof1:altsyncram6|     ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6                      ; work         ;
;       |fifo_adc:fifo_adc_inst_21|                   ; 181 (0)     ; 162          ; 8192        ; 2    ; 0    ; 0            ; 19 (0)       ; 72 (0)            ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21                                                                                                                       ; work         ;
;          |dcfifo:dcfifo_component|                  ; 181 (0)     ; 162          ; 8192        ; 2    ; 0    ; 0            ; 19 (0)       ; 72 (0)            ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component                                                                                               ; work         ;
;             |dcfifo_pdi1:auto_generated|            ; 181 (12)    ; 162          ; 8192        ; 2    ; 0    ; 0            ; 19 (2)       ; 72 (10)           ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated                                                                    ; work         ;
;                |a_fefifo_30d:read_state|            ; 9 (9)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 3 (3)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_fefifo_30d:read_state                                            ; work         ;
;                |a_fefifo_pdc:write_state|           ; 3 (3)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_fefifo_pdc:write_state                                           ; work         ;
;                |a_gray2bin_26b:gray2bin_rs_nbwp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_gray2bin_26b:gray2bin_rs_nbwp                                    ; work         ;
;                |a_gray2bin_26b:gray2bin_ws_nbrp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_gray2bin_26b:gray2bin_ws_nbrp                                    ; work         ;
;                |a_graycounter_626:rdptr_g|          ; 19 (19)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_graycounter_626:rdptr_g                                          ; work         ;
;                |a_graycounter_626:wrptr_g|          ; 18 (18)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 4 (4)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_graycounter_626:wrptr_g                                          ; work         ;
;                |alt_synch_pipe_0e8:dffpipe_rs_dgwp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_rs_dgwp                                 ; work         ;
;                   |dffpipe_qe9:dffpipe9|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_rs_dgwp|dffpipe_qe9:dffpipe9            ; work         ;
;                |alt_synch_pipe_0e8:dffpipe_ws_dgrp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp                                 ; work         ;
;                   |dffpipe_qe9:dffpipe9|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp|dffpipe_qe9:dffpipe9            ; work         ;
;                |cntr_kua:rdptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|cntr_kua:rdptr_b                                                   ; work         ;
;                |cntr_kua:wrptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|cntr_kua:wrptr_b                                                   ; work         ;
;                |dffpipe_oe9:dffpipe_rdbuw|          ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_rdbuw                                          ; work         ;
;                |dffpipe_oe9:dffpipe_rs_dbwp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_rs_dbwp                                        ; work         ;
;                |dffpipe_oe9:dffpipe_wr_dbuw|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_wr_dbuw                                        ; work         ;
;                |dffpipe_oe9:dffpipe_ws_nbrp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dffpipe_oe9:dffpipe_ws_nbrp                                        ; work         ;
;                |dpram_n3v:fiforam|                  ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam                                                  ; work         ;
;                   |altsyncram_pof1:altsyncram6|     ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6                      ; work         ;
;       |reg_8bits:reg_8bits_inst|                    ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|reg_8bits:reg_8bits_inst                                                                                                                        ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all:inst200|reg_8bits:reg_8bits_inst|lpm_ff:lpm_ff_component                                                                                                ; work         ;
;    |ADC_AD9220_all_CMS:inst182|                     ; 453 (54)    ; 352          ; 16384       ; 4    ; 0    ; 0            ; 101 (39)     ; 151 (6)           ; 201 (9)          ; 92 (0)          ; 28 (2)     ; |Skiroc2|ADC_AD9220_all_CMS:inst182                                                                                                                                             ; work         ;
;       |Read_Word:Read_Word2|                        ; 22 (22)     ; 0            ; 0           ; 0    ; 0    ; 0            ; 22 (22)      ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 16 (16)    ; |Skiroc2|ADC_AD9220_all_CMS:inst182|Read_Word:Read_Word2                                                                                                                        ; work         ;
;       |count2bits:counter_2b_inst|                  ; 2 (0)       ; 2            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 2 (0)            ; 2 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|count2bits:counter_2b_inst                                                                                                                  ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 2 (0)       ; 2            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 2 (0)            ; 2 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|count2bits:counter_2b_inst|lpm_counter:lpm_counter_component                                                                                ; work         ;
;             |cntr_cdj:auto_generated|               ; 2 (2)       ; 2            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 2 (2)            ; 2 (2)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|count2bits:counter_2b_inst|lpm_counter:lpm_counter_component|cntr_cdj:auto_generated                                                        ; work         ;
;       |counter_10b:counter_10b_inst|                ; 10 (0)      ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (0)           ; 10 (0)          ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|counter_10b:counter_10b_inst                                                                                                                ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 10 (0)      ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (0)           ; 10 (0)          ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|counter_10b:counter_10b_inst|lpm_counter:lpm_counter_component                                                                              ; work         ;
;             |cntr_chi:auto_generated|               ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|counter_10b:counter_10b_inst|lpm_counter:lpm_counter_component|cntr_chi:auto_generated                                                      ; work         ;
;       |fifo_acd_SK2CMS:fifo_adc_inst_20|            ; 183 (0)     ; 162          ; 8192        ; 2    ; 0    ; 0            ; 21 (0)       ; 72 (0)            ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20                                                                                                            ; work         ;
;          |dcfifo:dcfifo_component|                  ; 183 (0)     ; 162          ; 8192        ; 2    ; 0    ; 0            ; 21 (0)       ; 72 (0)            ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component                                                                                    ; work         ;
;             |dcfifo_elh1:auto_generated|            ; 183 (12)    ; 162          ; 8192        ; 2    ; 0    ; 0            ; 21 (2)       ; 72 (10)           ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated                                                         ; work         ;
;                |a_fefifo_ghc:read_state|            ; 9 (9)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 3 (3)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_fefifo_ghc:read_state                                 ; work         ;
;                |a_fefifo_pdc:write_state|           ; 3 (3)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_fefifo_pdc:write_state                                ; work         ;
;                |a_gray2bin_26b:gray2bin_rs_nbwp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_gray2bin_26b:gray2bin_rs_nbwp                         ; work         ;
;                |a_gray2bin_26b:gray2bin_ws_nbrp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_gray2bin_26b:gray2bin_ws_nbrp                         ; work         ;
;                |a_graycounter_626:rdptr_g|          ; 21 (21)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 7 (7)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_graycounter_626:rdptr_g                               ; work         ;
;                |a_graycounter_626:wrptr_g|          ; 18 (18)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 4 (4)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_graycounter_626:wrptr_g                               ; work         ;
;                |alt_synch_pipe_0e8:dffpipe_ws_dgrp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp                      ; work         ;
;                   |dffpipe_qe9:dffpipe9|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp|dffpipe_qe9:dffpipe9 ; work         ;
;                |alt_synch_pipe_1e8:dffpipe_rs_dgwp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_1e8:dffpipe_rs_dgwp                      ; work         ;
;                   |dffpipe_te9:dffpipe3|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_1e8:dffpipe_rs_dgwp|dffpipe_te9:dffpipe3 ; work         ;
;                |cntr_kua:rdptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|cntr_kua:rdptr_b                                        ; work         ;
;                |cntr_kua:wrptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|cntr_kua:wrptr_b                                        ; work         ;
;                |dffpipe_oe9:dffpipe_rdbuw|          ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_rdbuw                               ; work         ;
;                |dffpipe_oe9:dffpipe_rs_dbwp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_rs_dbwp                             ; work         ;
;                |dffpipe_oe9:dffpipe_wr_dbuw|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_wr_dbuw                             ; work         ;
;                |dffpipe_oe9:dffpipe_ws_nbrp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_ws_nbrp                             ; work         ;
;                |dpram_n3v:fiforam|                  ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam                                       ; work         ;
;                   |altsyncram_pof1:altsyncram6|     ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6           ; work         ;
;       |fifo_acd_SK2CMS:fifo_adc_inst_21|            ; 181 (0)     ; 162          ; 8192        ; 2    ; 0    ; 0            ; 19 (0)       ; 72 (0)            ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21                                                                                                            ; work         ;
;          |dcfifo:dcfifo_component|                  ; 181 (0)     ; 162          ; 8192        ; 2    ; 0    ; 0            ; 19 (0)       ; 72 (0)            ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component                                                                                    ; work         ;
;             |dcfifo_elh1:auto_generated|            ; 181 (12)    ; 162          ; 8192        ; 2    ; 0    ; 0            ; 19 (2)       ; 72 (10)           ; 90 (0)           ; 40 (0)          ; 5 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated                                                         ; work         ;
;                |a_fefifo_ghc:read_state|            ; 9 (9)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 3 (3)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_fefifo_ghc:read_state                                 ; work         ;
;                |a_fefifo_pdc:write_state|           ; 3 (3)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_fefifo_pdc:write_state                                ; work         ;
;                |a_gray2bin_26b:gray2bin_rs_nbwp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_gray2bin_26b:gray2bin_rs_nbwp                         ; work         ;
;                |a_gray2bin_26b:gray2bin_ws_nbrp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_gray2bin_26b:gray2bin_ws_nbrp                         ; work         ;
;                |a_graycounter_626:rdptr_g|          ; 19 (19)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_graycounter_626:rdptr_g                               ; work         ;
;                |a_graycounter_626:wrptr_g|          ; 18 (18)     ; 14           ; 0           ; 0    ; 0    ; 0            ; 4 (4)        ; 0 (0)             ; 14 (14)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_graycounter_626:wrptr_g                               ; work         ;
;                |alt_synch_pipe_0e8:dffpipe_ws_dgrp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp                      ; work         ;
;                   |dffpipe_qe9:dffpipe9|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_0e8:dffpipe_ws_dgrp|dffpipe_qe9:dffpipe9 ; work         ;
;                |alt_synch_pipe_1e8:dffpipe_rs_dgwp| ; 30 (0)      ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_1e8:dffpipe_rs_dgwp                      ; work         ;
;                   |dffpipe_te9:dffpipe3|            ; 30 (30)     ; 30           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 28 (28)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|alt_synch_pipe_1e8:dffpipe_rs_dgwp|dffpipe_te9:dffpipe3 ; work         ;
;                |cntr_kua:rdptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|cntr_kua:rdptr_b                                        ; work         ;
;                |cntr_kua:wrptr_b|                   ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|cntr_kua:wrptr_b                                        ; work         ;
;                |dffpipe_oe9:dffpipe_rdbuw|          ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_rdbuw                               ; work         ;
;                |dffpipe_oe9:dffpipe_rs_dbwp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_rs_dbwp                             ; work         ;
;                |dffpipe_oe9:dffpipe_wr_dbuw|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 10 (10)          ; 10 (10)         ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_wr_dbuw                             ; work         ;
;                |dffpipe_oe9:dffpipe_ws_nbrp|        ; 10 (10)     ; 10           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dffpipe_oe9:dffpipe_ws_nbrp                             ; work         ;
;                |dpram_n3v:fiforam|                  ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam                                       ; work         ;
;                   |altsyncram_pof1:altsyncram6|     ; 0 (0)       ; 0            ; 8192        ; 2    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6           ; work         ;
;       |reg_8bits:reg_8bits_inst|                    ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|reg_8bits:reg_8bits_inst                                                                                                                    ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|ADC_AD9220_all_CMS:inst182|reg_8bits:reg_8bits_inst|lpm_ff:lpm_ff_component                                                                                            ; work         ;
;    |AutoDAQ_SK2CMS_v1a:inst199|                     ; 50 (22)     ; 38           ; 0           ; 0    ; 0    ; 0            ; 12 (12)      ; 4 (3)             ; 34 (7)           ; 27 (0)          ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2CMS_v1a:inst199                                                                                                                                             ; work         ;
;       |count27bits:count27bit_inst|                 ; 27 (0)      ; 27           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 27 (0)           ; 27 (0)          ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2CMS_v1a:inst199|count27bits:count27bit_inst                                                                                                                 ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 27 (0)      ; 27           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 27 (0)           ; 27 (0)          ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2CMS_v1a:inst199|count27bits:count27bit_inst|lpm_counter:lpm_counter_component                                                                               ; work         ;
;             |cntr_khi:auto_generated|               ; 27 (27)     ; 27           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 27 (27)          ; 27 (27)         ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2CMS_v1a:inst199|count27bits:count27bit_inst|lpm_counter:lpm_counter_component|cntr_khi:auto_generated                                                       ; work         ;
;       |reg_8bits:reg_8bits_inst|                    ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2CMS_v1a:inst199|reg_8bits:reg_8bits_inst                                                                                                                    ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2CMS_v1a:inst199|reg_8bits:reg_8bits_inst|lpm_ff:lpm_ff_component                                                                                            ; work         ;
;    |AutoDAQ_SK2_v1:inst130|                         ; 31 (17)     ; 21           ; 0           ; 0    ; 0    ; 0            ; 10 (10)      ; 3 (2)             ; 18 (5)           ; 13 (0)          ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2_v1:inst130                                                                                                                                                 ; work         ;
;       |count16bits:count16bit_inst|                 ; 13 (0)      ; 13           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 13 (0)           ; 13 (0)          ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2_v1:inst130|count16bits:count16bit_inst                                                                                                                     ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 13 (0)      ; 13           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 13 (0)           ; 13 (0)          ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2_v1:inst130|count16bits:count16bit_inst|lpm_counter:lpm_counter_component                                                                                   ; work         ;
;             |cntr_ihi:auto_generated|               ; 13 (13)     ; 13           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 13 (13)          ; 13 (13)         ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2_v1:inst130|count16bits:count16bit_inst|lpm_counter:lpm_counter_component|cntr_ihi:auto_generated                                                           ; work         ;
;       |reg_8bits:reg_8bits_inst|                    ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2_v1:inst130|reg_8bits:reg_8bits_inst                                                                                                                        ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|AutoDAQ_SK2_v1:inst130|reg_8bits:reg_8bits_inst|lpm_ff:lpm_ff_component                                                                                                ; work         ;
;    |En_clk:inst82|                                  ; 8 (8)       ; 7            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 3 (3)             ; 4 (4)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|En_clk:inst82                                                                                                                                                          ; work         ;
;    |Firmware_v:inst14|                              ; 59 (0)      ; 0            ; 0           ; 0    ; 0    ; 0            ; 59 (0)       ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 42 (0)     ; |Skiroc2|Firmware_v:inst14                                                                                                                                                      ; work         ;
;       |Read_Word:Read_Word0|                        ; 59 (59)     ; 0            ; 0           ; 0    ; 0    ; 0            ; 59 (59)      ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 42 (42)    ; |Skiroc2|Firmware_v:inst14|Read_Word:Read_Word0                                                                                                                                 ; work         ;
;    |RSwithTimeOut:inst122|                          ; 7 (3)       ; 5            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 5 (1)            ; 5 (1)           ; 1 (1)      ; |Skiroc2|RSwithTimeOut:inst122                                                                                                                                                  ; work         ;
;       |count4timeout:count4timeout_inst|            ; 4 (0)       ; 4            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 4 (0)            ; 4 (0)           ; 0 (0)      ; |Skiroc2|RSwithTimeOut:inst122|count4timeout:count4timeout_inst                                                                                                                 ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 4 (0)       ; 4            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 4 (0)            ; 4 (0)           ; 0 (0)      ; |Skiroc2|RSwithTimeOut:inst122|count4timeout:count4timeout_inst|lpm_counter:lpm_counter_component                                                                               ; work         ;
;             |cntr_cvi:auto_generated|               ; 4 (4)       ; 4            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 4 (4)            ; 4 (4)           ; 0 (0)      ; |Skiroc2|RSwithTimeOut:inst122|count4timeout:count4timeout_inst|lpm_counter:lpm_counter_component|cntr_cvi:auto_generated                                                       ; work         ;
;    |Scurve_1input_16bits_sk2_cms:inst196|           ; 57 (14)     ; 37           ; 0           ; 0    ; 0    ; 0            ; 20 (14)      ; 1 (0)             ; 36 (0)           ; 32 (0)          ; 2 (2)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196                                                                                                                                   ; work         ;
;       |Read_Word:Read_Word18|                       ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|Read_Word:Read_Word18                                                                                                             ; work         ;
;       |Read_Word:Read_Word19|                       ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|Read_Word:Read_Word19                                                                                                             ; work         ;
;       |Read_Word:Read_Word8|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|Read_Word:Read_Word8                                                                                                              ; work         ;
;       |Read_Word:Read_Word9|                        ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|Read_Word:Read_Word9                                                                                                              ; work         ;
;       |count16bits:count8bits_pulse|                ; 16 (0)      ; 16           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 16 (0)           ; 16 (0)          ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|count16bits:count8bits_pulse                                                                                                      ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 16 (0)      ; 16           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 16 (0)           ; 16 (0)          ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|count16bits:count8bits_pulse|lpm_counter:lpm_counter_component                                                                    ; work         ;
;             |cntr_ihi:auto_generated|               ; 16 (16)     ; 16           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 16 (16)          ; 16 (16)         ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|count16bits:count8bits_pulse|lpm_counter:lpm_counter_component|cntr_ihi:auto_generated                                            ; work         ;
;       |count16bits:count8bits_trig|                 ; 16 (0)      ; 16           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 16 (0)           ; 16 (0)          ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|count16bits:count8bits_trig                                                                                                       ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 16 (0)      ; 16           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 16 (0)           ; 16 (0)          ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|count16bits:count8bits_trig|lpm_counter:lpm_counter_component                                                                     ; work         ;
;             |cntr_ihi:auto_generated|               ; 16 (16)     ; 16           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 16 (16)          ; 16 (16)         ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|count16bits:count8bits_trig|lpm_counter:lpm_counter_component|cntr_ihi:auto_generated                                             ; work         ;
;       |flipflopaclr:Sync1|                          ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:Sync1                                                                                                                ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:Sync1|lpm_ff:lpm_ff_component                                                                                        ; work         ;
;       |flipflopaclr:Sync2|                          ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:Sync2                                                                                                                ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:Sync2|lpm_ff:lpm_ff_component                                                                                        ; work         ;
;       |flipflopaclr:SyncEnd|                        ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncEnd                                                                                                              ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncEnd|lpm_ff:lpm_ff_component                                                                                      ; work         ;
;       |flipflopaclr:SyncTrig_1|                     ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncTrig_1                                                                                                           ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncTrig_1|lpm_ff:lpm_ff_component                                                                                   ; work         ;
;       |flipflopaclr:SyncTrig_2|                     ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncTrig_2                                                                                                           ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncTrig_2|lpm_ff:lpm_ff_component                                                                                   ; work         ;
;    |SlowControl_SK2_ERO:inst15|                     ; 283 (57)    ; 207          ; 2048        ; 1    ; 0    ; 0            ; 76 (43)      ; 61 (0)            ; 146 (14)         ; 36 (0)          ; 17 (3)     ; |Skiroc2|SlowControl_SK2_ERO:inst15                                                                                                                                             ; work         ;
;       |Read_Word:Read_Word0|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word0                                                                                                                        ; work         ;
;       |Read_Word:Read_Word1|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word1                                                                                                                        ; work         ;
;       |Read_Word:Read_Word2|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word2                                                                                                                        ; work         ;
;       |Read_Word:Read_Word3|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word3                                                                                                                        ; work         ;
;       |Read_Word:Read_Word4|                        ; 12 (12)     ; 0            ; 0           ; 0    ; 0    ; 0            ; 12 (12)      ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 9 (9)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word4                                                                                                                        ; work         ;
;       |Read_Word:Read_Word5|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word5                                                                                                                        ; work         ;
;       |Read_Word:Read_Word6|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word6                                                                                                                        ; work         ;
;       |Read_Word:Read_Word7|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|Read_Word:Read_Word7                                                                                                                        ; work         ;
;       |count4bits:count_shift|                      ; 4 (0)       ; 4            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 4 (0)            ; 4 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|count4bits:count_shift                                                                                                                      ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 4 (0)       ; 4            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 4 (0)            ; 4 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|count4bits:count_shift|lpm_counter:lpm_counter_component                                                                                    ; work         ;
;             |cntr_fui:auto_generated|               ; 4 (4)       ; 4            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 4 (4)            ; 4 (4)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|count4bits:count_shift|lpm_counter:lpm_counter_component|cntr_fui:auto_generated                                                            ; work         ;
;       |fifo:fifo_inst|                              ; 144 (0)     ; 130          ; 2048        ; 1    ; 0    ; 0            ; 14 (0)       ; 58 (0)            ; 72 (0)           ; 32 (0)          ; 5 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst                                                                                                                              ; work         ;
;          |dcfifo:dcfifo_component|                  ; 144 (0)     ; 130          ; 2048        ; 1    ; 0    ; 0            ; 14 (0)       ; 58 (0)            ; 72 (0)           ; 32 (0)          ; 5 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component                                                                                                      ; work         ;
;             |dcfifo_gai1:auto_generated|            ; 144 (10)    ; 130          ; 2048        ; 1    ; 0    ; 0            ; 14 (2)       ; 58 (8)            ; 72 (0)           ; 32 (0)          ; 5 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated                                                                           ; work         ;
;                |a_fefifo_6bc:write_state|           ; 3 (3)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_fefifo_6bc:write_state                                                  ; work         ;
;                |a_fefifo_tec:read_state|            ; 7 (7)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 4 (4)        ; 0 (0)             ; 3 (3)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_fefifo_tec:read_state                                                   ; work         ;
;                |a_gray2bin_p4b:gray2bin_rs_nbwp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_gray2bin_p4b:gray2bin_rs_nbwp                                           ; work         ;
;                |a_gray2bin_p4b:gray2bin_ws_nbrp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_gray2bin_p4b:gray2bin_ws_nbrp                                           ; work         ;
;                |a_graycounter_t06:rdptr_g|          ; 14 (14)     ; 11           ; 0           ; 0    ; 0    ; 0            ; 3 (3)        ; 0 (0)             ; 11 (11)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g                                                 ; work         ;
;                |a_graycounter_t06:wrptr_g|          ; 14 (14)     ; 11           ; 0           ; 0    ; 0    ; 0            ; 3 (3)        ; 0 (0)             ; 11 (11)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g                                                 ; work         ;
;                |alt_synch_pipe_nc8:dffpipe_rs_dgwp| ; 24 (0)      ; 24           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 22 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp                                        ; work         ;
;                   |dffpipe_hd9:dffpipe9|            ; 24 (24)     ; 24           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 22 (22)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9                   ; work         ;
;                |alt_synch_pipe_nc8:dffpipe_ws_dgrp| ; 24 (0)      ; 24           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 22 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp                                        ; work         ;
;                   |dffpipe_hd9:dffpipe9|            ; 24 (24)     ; 24           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 22 (22)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9                   ; work         ;
;                |cntr_bta:rdptr_b|                   ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 8 (8)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b                                                          ; work         ;
;                |cntr_bta:wrptr_b|                   ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 8 (8)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b                                                          ; work         ;
;                |dffpipe_fd9:dffpipe_rdbuw|          ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 8 (8)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw                                                 ; work         ;
;                |dffpipe_fd9:dffpipe_rs_dbwp|        ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 5 (5)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp                                               ; work         ;
;                |dffpipe_fd9:dffpipe_wr_dbuw|        ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 8 (8)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw                                               ; work         ;
;                |dffpipe_fd9:dffpipe_ws_nbrp|        ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 5 (5)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp                                               ; work         ;
;                |dpram_e2v:fiforam|                  ; 0 (0)       ; 0            ; 2048        ; 1    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dpram_e2v:fiforam                                                         ; work         ;
;                   |altsyncram_7mf1:altsyncram6|     ; 0 (0)       ; 0            ; 2048        ; 1    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dpram_e2v:fiforam|altsyncram_7mf1:altsyncram6                             ; work         ;
;       |flipflopaclr:flipflopaclr_instwr|            ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|flipflopaclr:flipflopaclr_instwr                                                                                                            ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|flipflopaclr:flipflopaclr_instwr|lpm_ff:lpm_ff_component                                                                                    ; work         ;
;       |flipflopaclr_en:flipflopaclr_en_instmemread| ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_en_instmemread                                                                                                 ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_en_instmemread|lpm_ff:lpm_ff_component                                                                         ; work         ;
;       |flipflopaclr_en:flipflopaclr_instmemsr|      ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_instmemsr                                                                                                      ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_instmemsr|lpm_ff:lpm_ff_component                                                                              ; work         ;
;       |latch_8:Ins0_7_Latch8|                       ; 56 (0)      ; 56           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (0)             ; 53 (0)           ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8                                                                                                                       ; work         ;
;          |reg_8bits:inst0_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 2 (0)             ; 6 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 2 (2)             ; 6 (6)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;          |reg_8bits:inst1_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 7 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;          |reg_8bits:inst2_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;          |reg_8bits:inst3_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;          |reg_8bits:inst5_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;          |reg_8bits:inst6_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;          |reg_8bits:inst7_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits                                                                                             ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component                                                                     ; work         ;
;    |TransmitRam:inst70|                             ; 230 (1)     ; 205          ; 32768       ; 8    ; 0    ; 0            ; 25 (0)       ; 93 (0)            ; 112 (1)          ; 52 (0)          ; 6 (0)      ; |Skiroc2|TransmitRam:inst70                                                                                                                                                     ; work         ;
;       |Read_Word:Read_Fifo_word_usedLSB|            ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|Read_Word:Read_Fifo_word_usedLSB                                                                                                                    ; work         ;
;       |Read_Word:Read_Fifo_word_usedMSB|            ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|Read_Word:Read_Fifo_word_usedMSB                                                                                                                    ; work         ;
;       |big_fifo:big_fifo_inst|                      ; 214 (0)     ; 192          ; 32768       ; 8    ; 0    ; 0            ; 22 (0)       ; 86 (0)            ; 106 (0)          ; 48 (0)          ; 6 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst                                                                                                                              ; work         ;
;          |dcfifo:dcfifo_component|                  ; 214 (0)     ; 192          ; 32768       ; 8    ; 0    ; 0            ; 22 (0)       ; 86 (0)            ; 106 (0)          ; 48 (0)          ; 6 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component                                                                                                      ; work         ;
;             |dcfifo_9ei1:auto_generated|            ; 214 (13)    ; 192          ; 32768       ; 8    ; 0    ; 0            ; 22 (1)       ; 86 (12)           ; 106 (0)          ; 48 (0)          ; 6 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated                                                                           ; work         ;
;                |a_fefifo_7ec:write_state|           ; 4 (4)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 3 (3)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_fefifo_7ec:write_state                                                  ; work         ;
;                |a_fefifo_h0d:read_state|            ; 8 (8)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 3 (3)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_fefifo_h0d:read_state                                                   ; work         ;
;                |a_gray2bin_46b:gray2bin_rs_nbwp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 3 (3)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_gray2bin_46b:gray2bin_rs_nbwp                                           ; work         ;
;                |a_gray2bin_46b:gray2bin_ws_nbrp|    ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_gray2bin_46b:gray2bin_ws_nbrp                                           ; work         ;
;                |a_graycounter_826:rdptr_g|          ; 24 (24)     ; 16           ; 0           ; 0    ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 16 (16)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_graycounter_826:rdptr_g                                                 ; work         ;
;                |a_graycounter_826:wrptr_g|          ; 21 (21)     ; 16           ; 0           ; 0    ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 16 (16)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_graycounter_826:wrptr_g                                                 ; work         ;
;                |alt_synch_pipe_2e8:dffpipe_rs_dgwp| ; 36 (0)      ; 36           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 33 (0)            ; 3 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|alt_synch_pipe_2e8:dffpipe_rs_dgwp                                        ; work         ;
;                   |dffpipe_se9:dffpipe9|            ; 36 (36)     ; 36           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 33 (33)           ; 3 (3)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|alt_synch_pipe_2e8:dffpipe_rs_dgwp|dffpipe_se9:dffpipe9                   ; work         ;
;                |alt_synch_pipe_2e8:dffpipe_ws_dgrp| ; 36 (0)      ; 36           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 34 (0)            ; 2 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|alt_synch_pipe_2e8:dffpipe_ws_dgrp                                        ; work         ;
;                   |dffpipe_se9:dffpipe9|            ; 36 (36)     ; 36           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 34 (34)           ; 2 (2)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|alt_synch_pipe_2e8:dffpipe_ws_dgrp|dffpipe_se9:dffpipe9                   ; work         ;
;                |cntr_mua:rdptr_b|                   ; 12 (12)     ; 12           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; 12 (12)         ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|cntr_mua:rdptr_b                                                          ; work         ;
;                |cntr_mua:wrptr_b|                   ; 12 (12)     ; 12           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; 12 (12)         ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|cntr_mua:wrptr_b                                                          ; work         ;
;                |dffpipe_re9:dffpipe_rdbuw|          ; 11 (11)     ; 11           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 11 (11)          ; 11 (11)         ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dffpipe_re9:dffpipe_rdbuw                                                 ; work         ;
;                |dffpipe_re9:dffpipe_rdusedw|        ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 1 (1)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dffpipe_re9:dffpipe_rdusedw                                               ; work         ;
;                |dffpipe_re9:dffpipe_rs_dbwp|        ; 12 (12)     ; 12           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (4)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dffpipe_re9:dffpipe_rs_dbwp                                               ; work         ;
;                |dffpipe_re9:dffpipe_wr_dbuw|        ; 12 (12)     ; 12           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; 12 (12)         ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dffpipe_re9:dffpipe_wr_dbuw                                               ; work         ;
;                |dffpipe_re9:dffpipe_ws_nbrp|        ; 12 (12)     ; 12           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 9 (9)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dffpipe_re9:dffpipe_ws_nbrp                                               ; work         ;
;                |dpram_p3v:fiforam|                  ; 0 (0)       ; 0            ; 32768       ; 8    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dpram_p3v:fiforam                                                         ; work         ;
;                   |altsyncram_tof1:altsyncram6|     ; 0 (0)       ; 0            ; 32768       ; 8    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dpram_p3v:fiforam|altsyncram_tof1:altsyncram6                             ; work         ;
;       |data_count:data_count_inst|                  ; 3 (0)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (0)            ; 3 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|data_count:data_count_inst                                                                                                                          ; work         ;
;          |lpm_counter:lpm_counter_component|        ; 3 (0)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (0)            ; 3 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|data_count:data_count_inst|lpm_counter:lpm_counter_component                                                                                        ; work         ;
;             |cntr_eui:auto_generated|               ; 3 (3)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (3)            ; 3 (3)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|data_count:data_count_inst|lpm_counter:lpm_counter_component|cntr_eui:auto_generated                                                                ; work         ;
;       |flipflop:delay_carry_inst|                   ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 1 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|flipflop:delay_carry_inst                                                                                                                           ; work         ;
;          |lpm_ff:lpm_ff_component|                  ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 1 (1)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|flipflop:delay_carry_inst|lpm_ff:lpm_ff_component                                                                                                   ; work         ;
;       |shift8register:shift8register_inst|          ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 7 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|shift8register:shift8register_inst                                                                                                                  ; work         ;
;          |lpm_shiftreg:lpm_shiftreg_component|      ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 7 (7)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|TransmitRam:inst70|shift8register:shift8register_inst|lpm_shiftreg:lpm_shiftreg_component                                                                              ; work         ;
;    |busmux:inst101|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst101                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst101|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst101|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst102|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst102                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst102|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst102|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst103|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst103                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst103|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst103|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst104|                                 ; 5 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 5 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst104                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 5 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 5 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst104|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 5 (5)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst104|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst105|                                 ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst105                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst105|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst105|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst106|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst106                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst106|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst106|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst107|                                 ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst107                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst107|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst107|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst109|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst109                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst109|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst109|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst115|                                 ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst115                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst115|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst115|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst118|                                 ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst118                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst118|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst118|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst128|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst128                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst128|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst128|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst129|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst129                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst129|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst129|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst139|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst139                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst139|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst139|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst148|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst148                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst148|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst148|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst150|                                 ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst150                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst150|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst150|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst151|                                 ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst151                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst151|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst151|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst154|                                 ; 6 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 6 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst154                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 6 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 6 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst154|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_rgc:auto_generated|                   ; 6 (6)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst154|lpm_mux:$00000|mux_rgc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst155|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (0)      ; |Skiroc2|busmux:inst155                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (0)      ; |Skiroc2|busmux:inst155|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|busmux:inst155|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst160|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst160                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst160|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst160|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst163|                                 ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst163                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst163|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst163|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst164|                                 ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst164                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst164|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst164|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst166|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst166                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst166|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst166|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst171|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst171                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst171|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst171|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst173|                                 ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst173                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst173|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst173|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst174|                                 ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst174                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst174|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst174|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst175|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst175                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst175|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst175|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst178|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst178                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst178|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst178|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst192|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst192                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst192|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst192|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst193|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst193                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst193|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst193|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst194|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst194                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst194|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst194|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst195|                                 ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst195                                                                                                                                                         ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst195|lpm_mux:$00000                                                                                                                                          ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst195|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                   ; work         ;
;    |busmux:inst72|                                  ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst72                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst72|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst72|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst73|                                  ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst73                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst73|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst73|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst74|                                  ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst74                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst74|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst74|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst76|                                  ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst76                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst76|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst76|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst81|                                  ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst81                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst81|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst81|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst88|                                  ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst88                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst88|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst88|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst89|                                  ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst89                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst89|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst89|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst90|                                  ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst90                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (0)      ; |Skiroc2|busmux:inst90|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|busmux:inst90|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst95|                                  ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst95                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 1 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst95|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst95|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst96|                                  ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst96                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 2 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst96|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst96|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |busmux:inst97|                                  ; 3 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 3 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst97                                                                                                                                                          ; work         ;
;       |lpm_mux:$00000|                              ; 3 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 3 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst97|lpm_mux:$00000                                                                                                                                           ; work         ;
;          |mux_3fc:auto_generated|                   ; 3 (3)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 3 (3)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|busmux:inst97|lpm_mux:$00000|mux_3fc:auto_generated                                                                                                                    ; work         ;
;    |clk_div:inst145|                                ; 3 (0)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (0)            ; 3 (0)           ; 0 (0)      ; |Skiroc2|clk_div:inst145                                                                                                                                                        ; work         ;
;       |lpm_counter:lpm_counter_component|           ; 3 (0)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (0)            ; 3 (0)           ; 0 (0)      ; |Skiroc2|clk_div:inst145|lpm_counter:lpm_counter_component                                                                                                                      ; work         ;
;          |cntr_crh:auto_generated|                  ; 3 (3)       ; 3            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (3)            ; 3 (3)           ; 0 (0)      ; |Skiroc2|clk_div:inst145|lpm_counter:lpm_counter_component|cntr_crh:auto_generated                                                                                              ; work         ;
;    |clk_div:inst2|                                  ; 6 (0)       ; 6            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 6 (0)            ; 6 (0)           ; 0 (0)      ; |Skiroc2|clk_div:inst2                                                                                                                                                          ; work         ;
;       |lpm_counter:lpm_counter_component|           ; 6 (0)       ; 6            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 6 (0)            ; 6 (0)           ; 0 (0)      ; |Skiroc2|clk_div:inst2|lpm_counter:lpm_counter_component                                                                                                                        ; work         ;
;          |cntr_crh:auto_generated|                  ; 6 (6)       ; 6            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 6 (6)            ; 6 (6)           ; 0 (0)      ; |Skiroc2|clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated                                                                                                ; work         ;
;    |delay_OR_trigger:inst1|                         ; 256 (0)     ; 256          ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 159 (0)           ; 97 (0)           ; 0 (0)           ; 0 (0)      ; |Skiroc2|delay_OR_trigger:inst1                                                                                                                                                 ; work         ;
;       |lpm_shiftreg:lpm_shiftreg_component|         ; 256 (256)   ; 256          ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 159 (159)         ; 97 (97)          ; 0 (0)           ; 0 (0)      ; |Skiroc2|delay_OR_trigger:inst1|lpm_shiftreg:lpm_shiftreg_component                                                                                                             ; work         ;
;    |delay_mux:inst120|                              ; 96 (0)      ; 0            ; 0           ; 0    ; 0    ; 0            ; 96 (0)       ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 98 (0)     ; |Skiroc2|delay_mux:inst120                                                                                                                                                      ; work         ;
;       |lpm_mux:lpm_mux_component|                   ; 96 (0)      ; 0            ; 0           ; 0    ; 0    ; 0            ; 96 (0)       ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 98 (0)     ; |Skiroc2|delay_mux:inst120|lpm_mux:lpm_mux_component                                                                                                                            ; work         ;
;          |mux_0vd:auto_generated|                   ; 96 (96)     ; 0            ; 0           ; 0    ; 0    ; 0            ; 96 (96)      ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 98 (98)    ; |Skiroc2|delay_mux:inst120|lpm_mux:lpm_mux_component|mux_0vd:auto_generated                                                                                                     ; work         ;
;    |flipflop:inst111|                               ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst111                                                                                                                                                       ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst111|lpm_ff:lpm_ff_component                                                                                                                               ; work         ;
;    |flipflop:inst58|                                ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst58                                                                                                                                                        ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst58|lpm_ff:lpm_ff_component                                                                                                                                ; work         ;
;    |flipflop:inst59|                                ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst59                                                                                                                                                        ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst59|lpm_ff:lpm_ff_component                                                                                                                                ; work         ;
;    |flipflop:inst60|                                ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst60                                                                                                                                                        ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst60|lpm_ff:lpm_ff_component                                                                                                                                ; work         ;
;    |flipflop:inst80|                                ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst80                                                                                                                                                        ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst80|lpm_ff:lpm_ff_component                                                                                                                                ; work         ;
;    |flipflop:inst85|                                ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst85                                                                                                                                                        ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst85|lpm_ff:lpm_ff_component                                                                                                                                ; work         ;
;    |flipflop:inst86|                                ; 1 (0)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst86                                                                                                                                                        ; work         ;
;       |lpm_ff:lpm_ff_component|                     ; 1 (1)       ; 1            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|flipflop:inst86|lpm_ff:lpm_ff_component                                                                                                                                ; work         ;
;    |mux4_1:inst143|                                 ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (0)      ; |Skiroc2|mux4_1:inst143                                                                                                                                                         ; work         ;
;       |lpm_mux:lpm_mux_component|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (0)      ; |Skiroc2|mux4_1:inst143|lpm_mux:lpm_mux_component                                                                                                                               ; work         ;
;          |mux_6fc:auto_generated|                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 2 (2)      ; |Skiroc2|mux4_1:inst143|lpm_mux:lpm_mux_component|mux_6fc:auto_generated                                                                                                        ; work         ;
;    |pll_sk2:inst|                                   ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|pll_sk2:inst                                                                                                                                                           ; work         ;
;       |altpll:altpll_component|                     ; 0 (0)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|pll_sk2:inst|altpll:altpll_component                                                                                                                                   ; work         ;
;    |static_8bit_registers:inst124|                  ; 82 (9)      ; 64           ; 0           ; 0    ; 0    ; 0            ; 18 (9)       ; 20 (0)            ; 44 (0)           ; 0 (0)           ; 1 (0)      ; |Skiroc2|static_8bit_registers:inst124                                                                                                                                          ; work         ;
;       |Read_Word:Read_Word0|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word0                                                                                                                     ; work         ;
;       |Read_Word:Read_Word1|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word1                                                                                                                     ; work         ;
;       |Read_Word:Read_Word2|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word2                                                                                                                     ; work         ;
;       |Read_Word:Read_Word3|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word3                                                                                                                     ; work         ;
;       |Read_Word:Read_Word4|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word4                                                                                                                     ; work         ;
;       |Read_Word:Read_Word5|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word5                                                                                                                     ; work         ;
;       |Read_Word:Read_Word6|                        ; 1 (1)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word6                                                                                                                     ; work         ;
;       |Read_Word:Read_Word7|                        ; 2 (2)       ; 0            ; 0           ; 0    ; 0    ; 0            ; 2 (2)        ; 0 (0)             ; 0 (0)            ; 0 (0)           ; 1 (1)      ; |Skiroc2|static_8bit_registers:inst124|Read_Word:Read_Word7                                                                                                                     ; work         ;
;       |latch_8:Ins0_7_Latch8|                       ; 64 (0)      ; 64           ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 20 (0)            ; 44 (0)           ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8                                                                                                                    ; work         ;
;          |reg_8bits:inst0_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst1_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 8 (8)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst2_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (0)             ; 4 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (4)             ; 4 (4)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst3_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (0)             ; 4 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (4)             ; 4 (4)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst4_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (0)             ; 4 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (4)             ; 4 (4)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst5_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (0)             ; 4 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 4 (4)             ; 4 (4)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst6_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (0)             ; 5 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 3 (3)             ; 5 (5)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;          |reg_8bits:inst7_reg_8bits|                ; 8 (0)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (0)             ; 7 (0)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits                                                                                          ; work         ;
;             |lpm_ff:lpm_ff_component|               ; 8 (8)       ; 8            ; 0           ; 0    ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 7 (7)            ; 0 (0)           ; 0 (0)      ; |Skiroc2|static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component                                                                  ; work         ;
;    |usb_full_interface_v:inst10|                    ; 288 (12)    ; 183          ; 0           ; 0    ; 0    ; 0            ; 105 (4)      ; 27 (2)            ; 156 (6)          ; 50 (0)          ; 46 (20)    ; |Skiroc2|usb_full_interface_v:inst10                                                                                                                                            ; work         ;
;       |interruptunit:m_interruptunit|               ; 33 (33)     ; 23           ; 0           ; 0    ; 0    ; 0            ; 10 (10)      ; 1 (1)             ; 22 (22)          ; 0 (0)           ; 1 (1)      ; |Skiroc2|usb_full_interface_v:inst10|interruptunit:m_interruptunit                                                                                                              ; work         ;
;       |readrequnit:m_readrequnit|                   ; 19 (19)     ; 16           ; 0           ; 0    ; 0    ; 0            ; 3 (3)        ; 1 (1)             ; 15 (15)          ; 0 (0)           ; 1 (1)      ; |Skiroc2|usb_full_interface_v:inst10|readrequnit:m_readrequnit                                                                                                                  ; work         ;
;       |rxunit:m_rxunit|                             ; 107 (107)   ; 73           ; 0           ; 0    ; 0    ; 0            ; 34 (34)      ; 17 (17)           ; 56 (56)          ; 17 (17)         ; 5 (5)      ; |Skiroc2|usb_full_interface_v:inst10|rxunit:m_rxunit                                                                                                                            ; work         ;
;       |txunit:m_txunit|                             ; 117 (117)   ; 63           ; 0           ; 0    ; 0    ; 0            ; 54 (54)      ; 6 (6)             ; 57 (57)          ; 33 (33)         ; 19 (19)    ; |Skiroc2|usb_full_interface_v:inst10|txunit:m_txunit                                                                                                                            ; work         ;
+-----------------------------------------------------+-------------+--------------+-------------+------+------+--------------+--------------+-------------------+------------------+-----------------+------------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+--------------+
Note: For table entries with two numbers listed, the numbers in parentheses indicate the number of resources of the given type used by the specific entity alone. The numbers listed outside of parentheses indicate the total resources of the given type used by the specific entity and all of its sub-entities in the hierarchy.


+----------------------------------------------------------------------------------------------+
; Delay Chain Summary                                                                          ;
+---------------------+----------+---------------+---------------+-----------------------+-----+
; Name                ; Pin Type ; Pad to Core 0 ; Pad to Core 1 ; Pad to Input Register ; TCO ;
+---------------------+----------+---------------+---------------+-----------------------+-----+
; XTIN                ; Input    ; OFF           ; OFF           ; --                    ; --  ;
; pwr_reset           ; Input    ; ON            ; ON            ; --                    ; --  ;
; IN_ALTERA5          ; Input    ; ON            ; ON            ; --                    ; --  ;
; end_readout1        ; Input    ; ON            ; ON            ; --                    ; --  ;
; IN_ALTERA3          ; Input    ; ON            ; ON            ; --                    ; --  ;
; IN_ALTERA1          ; Input    ; ON            ; ON            ; --                    ; --  ;
; IN_ALTERA2          ; Input    ; ON            ; ON            ; --                    ; --  ;
; IN_ALTERA4          ; Input    ; ON            ; ON            ; --                    ; --  ;
; digital_probe1      ; Input    ; ON            ; ON            ; --                    ; --  ;
; digital_probe2      ; Input    ; ON            ; ON            ; --                    ; --  ;
; TrigOutb            ; Input    ; ON            ; ON            ; --                    ; --  ;
; end_readout2        ; Input    ; ON            ; ON            ; --                    ; --  ;
; IN_ALTERA6          ; Input    ; ON            ; ON            ; --                    ; --  ;
; sr_out              ; Input    ; ON            ; ON            ; --                    ; --  ;
; srout_read          ; Input    ; ON            ; ON            ; --                    ; --  ;
; ChipSatb            ; Input    ; ON            ; ON            ; --                    ; --  ;
; clk_gene_ext        ; Input    ; ON            ; ON            ; --                    ; --  ;
; hold_conn           ; Input    ; ON            ; ON            ; --                    ; --  ;
; clk_osc             ; Input    ; --            ; --            ; --                    ; --  ;
; ADC[5]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[4]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; OTR                 ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[2]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[10]             ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[0]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[8]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[1]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[9]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[3]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[11]             ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[7]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; ADC[6]              ; Input    ; ON            ; ON            ; --                    ; --  ;
; TransmitOn1b        ; Input    ; ON            ; ON            ; --                    ; --  ;
; TransmitOn2b        ; Input    ; ON            ; ON            ; --                    ; --  ;
; Dout2b              ; Input    ; ON            ; ON            ; --                    ; --  ;
; Dout1b              ; Input    ; ON            ; ON            ; --                    ; --  ;
; nTXE                ; Input    ; ON            ; ON            ; --                    ; --  ;
; nRXF                ; Input    ; ON            ; ON            ; --                    ; --  ;
; adc_clk             ; Output   ; --            ; --            ; --                    ; --  ;
; resetb              ; Output   ; --            ; --            ; --                    ; --  ;
; start_acq           ; Output   ; --            ; --            ; --                    ; --  ;
; R_C                 ; Output   ; --            ; --            ; --                    ; --  ;
; start_readout2      ; Output   ; --            ; --            ; --                    ; --  ;
; start_readout1      ; Output   ; --            ; --            ; --                    ; --  ;
; rstb_pa             ; Output   ; --            ; --            ; --                    ; --  ;
; ck_read             ; Output   ; --            ; --            ; --                    ; --  ;
; srin_read           ; Output   ; --            ; --            ; --                    ; --  ;
; pwr_on_a            ; Output   ; --            ; --            ; --                    ; --  ;
; pwr_on_adc          ; Output   ; --            ; --            ; --                    ; --  ;
; pwr_on_dac          ; Output   ; --            ; --            ; --                    ; --  ;
; pwr_on_d            ; Output   ; --            ; --            ; --                    ; --  ;
; sr_in               ; Output   ; --            ; --            ; --                    ; --  ;
; sr_rstb             ; Output   ; --            ; --            ; --                    ; --  ;
; sr_ck               ; Output   ; --            ; --            ; --                    ; --  ;
; select              ; Output   ; --            ; --            ; --                    ; --  ;
; SYNC_GENE           ; Output   ; --            ; --            ; --                    ; --  ;
; test16              ; Output   ; --            ; --            ; --                    ; --  ;
; start_convb         ; Output   ; --            ; --            ; --                    ; --  ;
; 40M_test            ; Output   ; --            ; --            ; --                    ; --  ;
; start_rampb_adc_ext ; Output   ; --            ; --            ; --                    ; --  ;
; start_ramp_tdc_ext  ; Output   ; --            ; --            ; --                    ; --  ;
; 5M                  ; Output   ; --            ; --            ; --                    ; --  ;
; hold                ; Output   ; --            ; --            ; --                    ; --  ;
; 40M                 ; Output   ; --            ; --            ; --                    ; --  ;
; V_E                 ; Output   ; --            ; --            ; --                    ; --  ;
; T_E                 ; Output   ; --            ; --            ; --                    ; --  ;
; out_altera1         ; Output   ; --            ; --            ; --                    ; --  ;
; out_altera2         ; Output   ; --            ; --            ; --                    ; --  ;
; out_altera3         ; Output   ; --            ; --            ; --                    ; --  ;
; out_altera4         ; Output   ; --            ; --            ; --                    ; --  ;
; out_altera5         ; Output   ; --            ; --            ; --                    ; --  ;
; out_altera6         ; Output   ; --            ; --            ; --                    ; --  ;
; WR                  ; Output   ; --            ; --            ; --                    ; --  ;
; nRD                 ; Output   ; --            ; --            ; --                    ; --  ;
; test40              ; Output   ; --            ; --            ; --                    ; --  ;
; test39              ; Output   ; --            ; --            ; --                    ; --  ;
; test38              ; Output   ; --            ; --            ; --                    ; --  ;
; test37              ; Output   ; --            ; --            ; --                    ; --  ;
; test36              ; Output   ; --            ; --            ; --                    ; --  ;
; test35              ; Output   ; --            ; --            ; --                    ; --  ;
; test34              ; Output   ; --            ; --            ; --                    ; --  ;
; test33              ; Output   ; --            ; --            ; --                    ; --  ;
; test32              ; Output   ; --            ; --            ; --                    ; --  ;
; test31              ; Output   ; --            ; --            ; --                    ; --  ;
; test1               ; Output   ; --            ; --            ; --                    ; --  ;
; test2               ; Output   ; --            ; --            ; --                    ; --  ;
; test3               ; Output   ; --            ; --            ; --                    ; --  ;
; test4               ; Output   ; --            ; --            ; --                    ; --  ;
; test5               ; Output   ; --            ; --            ; --                    ; --  ;
; test6               ; Output   ; --            ; --            ; --                    ; --  ;
; test7               ; Output   ; --            ; --            ; --                    ; --  ;
; test8               ; Output   ; --            ; --            ; --                    ; --  ;
; test9               ; Output   ; --            ; --            ; --                    ; --  ;
; test10              ; Output   ; --            ; --            ; --                    ; --  ;
; test11              ; Output   ; --            ; --            ; --                    ; --  ;
; test12              ; Output   ; --            ; --            ; --                    ; --  ;
; test13              ; Output   ; --            ; --            ; --                    ; --  ;
; test14              ; Output   ; --            ; --            ; --                    ; --  ;
; test15              ; Output   ; --            ; --            ; --                    ; --  ;
; test17              ; Output   ; --            ; --            ; --                    ; --  ;
; test18              ; Output   ; --            ; --            ; --                    ; --  ;
; test19              ; Output   ; --            ; --            ; --                    ; --  ;
; test20              ; Output   ; --            ; --            ; --                    ; --  ;
; test21              ; Output   ; --            ; --            ; --                    ; --  ;
; test22              ; Output   ; --            ; --            ; --                    ; --  ;
; test23              ; Output   ; --            ; --            ; --                    ; --  ;
; test24              ; Output   ; --            ; --            ; --                    ; --  ;
; test25              ; Output   ; --            ; --            ; --                    ; --  ;
; test26              ; Output   ; --            ; --            ; --                    ; --  ;
; test27              ; Output   ; --            ; --            ; --                    ; --  ;
; test28              ; Output   ; --            ; --            ; --                    ; --  ;
; test29              ; Output   ; --            ; --            ; --                    ; --  ;
; test30              ; Output   ; --            ; --            ; --                    ; --  ;
; PLL_OUT             ; Output   ; --            ; --            ; --                    ; --  ;
; LED                 ; Output   ; --            ; --            ; --                    ; --  ;
; DAQ11               ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ4                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; USB[7]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[6]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[5]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[4]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[3]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[2]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[1]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; USB[0]              ; Bidir    ; ON            ; ON            ; --                    ; --  ;
; DAQ12               ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ9                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ0                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ2                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ3                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ5                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ7                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ6                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ8                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ1                ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; DAQ10               ; Bidir    ; OFF           ; OFF           ; --                    ; --  ;
; R_C(n)              ; Output   ; --            ; --            ; --                    ; --  ;
; 5M(n)               ; Output   ; --            ; --            ; --                    ; --  ;
; 40M(n)              ; Output   ; --            ; --            ; --                    ; --  ;
; V_E(n)              ; Output   ; --            ; --            ; --                    ; --  ;
; T_E(n)              ; Output   ; --            ; --            ; --                    ; --  ;
+---------------------+----------+---------------+---------------+-----------------------+-----+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Pad To Core Delay Chain Fanout                                                                                                                                                                                 ;
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------------+---------+
; Source Pin / Fanout                                                                                                                                                              ; Pad To Core Index ; Setting ;
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------------+---------+
; XTIN                                                                                                                                                                             ;                   ;         ;
; pwr_reset                                                                                                                                                                        ;                   ;         ;
;      - ADC_AD9220_all_CMS:inst182|temp1                                                                                                                                          ; 1                 ; ON      ;
;      - clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella1                                                                                    ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|WR                                                                                                                            ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rd                                                                                                                            ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|busyreadreq                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|user_interrupt                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|n_read                                                                                                                        ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|n_read                                                                                                              ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|n_read                                                                                                          ; 1                 ; ON      ;
;      - RSwithTimeOut:inst122|reset_RShold                                                                                                                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_instmemsr|lpm_ff:lpm_ff_component|dffs[0]                                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|StateMachine[0]                                                                                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|StateMachine[1]                                                                                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|StateMachine[2]                                                                                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|StateMachine[3]                                                                                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_en_instmemread|lpm_ff:lpm_ff_component|dffs[0]                                                                    ; 1                 ; ON      ;
;      - pll_sk2:inst|altpll:altpll_component|pll                                                                                                                                  ; 1                 ; ON      ;
;      - inst77                                                                                                                                                                    ; 1                 ; ON      ;
;      - inst183                                                                                                                                                                   ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|Read_Word:Read_Word7|User_Data[7]~0                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|end_write_r2                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|n_write                                                                                                                       ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|user_data[7]~3                                                                                                                                 ; 1                 ; ON      ;
;      - inst218                                                                                                                                                                   ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella3                                                                                    ; 1                 ; ON      ;
;      - clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella0                                                                                    ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella4                                                                                    ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00001                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte_ok_s                                                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|txe_latch                                                                                                                     ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10000                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10011                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|rd_data_ok_s                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00101                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|end_data                                                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10100                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.01001                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|header_error_latch_2                                                                                            ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|trailer_error_latch                                                                                             ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_latch                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|runtx                                                                                                               ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|busyrx                                                                                                                        ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00000                                                                                                         ; 1                 ; ON      ;
;      - clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella2                                                                                    ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rxf_latch                                                                                                                     ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|datavalid                                                                                                                     ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0000                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|read_write                                                                                                                    ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0111                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|end_write_r1                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|end_data                                                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0101                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1011                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0010                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|header_ok                                                                                                                     ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|read_req_latch                                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_presentstate.000                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|rdreq_presentstate.01                                                                                               ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|rdreq_presentstate.10                                                                                               ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb_ok_s                                                                                                       ; 1                 ; ON      ;
;      - clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella5                                                                                    ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - inst170                                                                                                                                                                   ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|flipflopaclr:flipflopaclr_instwr|lpm_ff:lpm_ff_component|dffs[0]                                                                               ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_fefifo_6bc:write_state|b_full                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_fefifo_tec:read_state|b_non_empty                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[0]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[1]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[2]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[3]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[4]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[5]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[6]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|counter5a[7]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[0]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[1]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[2]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[3]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[4]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[5]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[6]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|counter5a[7]                                       ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|comb~0                                                                                                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|mem_startcycle~0                                                                                                                               ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|Shift_order[3]                                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|end_write_s                                                                                                                   ; 1                 ; ON      ;
;      - clk_div:inst145|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella2                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_presentstate.001                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_presentstate.010                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txe_r1                                                                                                                                        ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|TXE_r                                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.01101                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00100                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[2]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[1]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[4]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[3]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[0]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[6]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[5]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[8]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[7]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[10]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[9]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[12]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[11]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[14]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[13]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[16]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[15]                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|header_error_latch                                                                                              ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|header_error_latch_r                                                                                            ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|trailer_error                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|read_req_r2                                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|trailer_ok                                                                                                                    ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1101                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1110                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0011                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rxf_r                                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptdatavalid[1]                                                                                                               ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptdatavalid[0]                                                                                                               ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[1]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[0]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[3]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[2]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[5]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[4]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[7]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[6]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|cptNdata[8]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|header_error                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10110                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.01010                                                                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[2]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[3]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[0]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[1]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[4]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[5]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[6]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_wr_dbuw|dffe8a[7]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[2]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[3]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[4]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[5]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[6]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[7]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[1]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rdbuw|dffe8a[0]                                          ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_fefifo_tec:read_state|b_one                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|parity3                                            ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|parity3                                            ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[7]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[6]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[5]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[4]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[3]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[2]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[1]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|usb_data[0]                                                                                                                   ; 1                 ; ON      ;
;      - clk_div:inst145|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella1                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[1]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[2]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[3]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[4]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[5]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[6]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[7]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[0]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[1]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[2]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[3]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[4]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[5]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[6]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataMsb[7]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interrupt_r1                                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxf_r1                                                                                                                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella2                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[2]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella3                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[3]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella0                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[0]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella1                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[1]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella4                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[4]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella5                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[5]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella6                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[6]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:wrptr_b|counter_cella7                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_ws_nbrp|dffe8a[7]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella2                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[2]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella3                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[3]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella4                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[4]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella5                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[5]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella6                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[6]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella7                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[7]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella1                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[1]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|cntr_bta:rdptr_b|counter_cella0                                              ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dffpipe_fd9:dffpipe_rs_dbwp|dffe8a[0]                                        ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|sub_parity4a0                                      ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:wrptr_g|sub_parity4a1                                      ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|sub_parity4a0                                      ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_graycounter_t06:rdptr_g|sub_parity4a1                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[7]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[6]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[5]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[5]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[4]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[3]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[3]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[2]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[1]                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[1]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[0]                                                                                                  ; 1                 ; ON      ;
;      - clk_div:inst145|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella0                                                                                  ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[7]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[6]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[5]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[3]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[2]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[0]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[7]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[6]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[5]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[3]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[2]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[0]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[7]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[6]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[5]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[4]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[3]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[2]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[1]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe11a[0]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[7]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[6]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[5]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[4]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[3]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[2]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[1]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe11a[0]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[7]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[6]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[5]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[4]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[3]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[2]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[1]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe10a[0]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[7]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[6]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[5]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[4]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[3]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[2]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[1]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe10a[0]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[7]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[6]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[5]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[4]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[3]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[2]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[1]                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|write_delay_cycle[0]                                                         ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|mem_startcycle~7                                                                                                                               ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|Hit_storage~2                                                                                                                                  ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[4]                                                                                                                     ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst4_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[1]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[2]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[0]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[3]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[4]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[5]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[6]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|NdataLsb[7]                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00110                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10001                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00010                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[3]                                                                                                                     ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[4]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[4]           ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[6]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[4]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[2]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[0]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[2]                                                                                                                     ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|Shift_order[0]                                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[5]                                                                                                                     ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[1]                                                                                                                     ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|a_fefifo_tec:read_state|llreq                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|data_latch[7]                                                                                                                 ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_ws_dgrp|dffpipe_hd9:dffpipe9|dffe12a[1]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|alt_synch_pipe_nc8:dffpipe_rs_dgwp|dffpipe_hd9:dffpipe9|dffe12a[1]           ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[0]                                                                                                                     ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|subadd[6]                                                                                                                     ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                             ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|n_write_r                                                                                                                                     ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1001                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[4]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[6]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[5]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[0]                                                                                                                 ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[2]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[3]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.01110                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|n_read_r                                                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1000                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0001                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[1]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_presentstate.011                                                                                      ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.01000                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|runtx                                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.01111                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1100                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0100                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1010                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|endtx                                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|n_read_r                                                                                                        ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10101                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|endinterrupt                                                                                                                  ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|NdataLsb[0]                                                                                                                   ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0110                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_presentstate.100                                                                                      ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txe_r2                                                                                                                                        ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00011                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.00111                                                                                                         ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxf_r2                                                                                                                                        ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|interruptunit:m_interruptunit|interrupt_r                                                                                                     ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|WR_r                                                                                                                                          ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10010                                                                                                         ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[7]                                                                                                                 ; 1                 ; ON      ;
;      - usb_full_interface_v:inst10|readrequnit:m_readrequnit|n_read_r                                                                                                            ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                             ; 1                 ; ON      ;
;      - static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                             ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                                                ; 1                 ; ON      ;
; IN_ALTERA5                                                                                                                                                                       ;                   ;         ;
;      - inst189~0                                                                                                                                                                 ; 1                 ; ON      ;
; end_readout1                                                                                                                                                                     ;                   ;         ;
;      - inst189~0                                                                                                                                                                 ; 0                 ; ON      ;
;      - AutoDAQ_SK2CMS_v1a:inst199|Mux12~2                                                                                                                                        ; 0                 ; ON      ;
;      - AutoDAQ_SK2CMS_v1a:inst199|Mux9~0                                                                                                                                         ; 0                 ; ON      ;
;      - AutoDAQ_SK2_v1:inst130|Mux3~1                                                                                                                                             ; 0                 ; ON      ;
;      - AutoDAQ_SK2_v1:inst130|Mux13~2                                                                                                                                            ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|ERO1                                                                                                                                           ; 0                 ; ON      ;
; IN_ALTERA3                                                                                                                                                                       ;                   ;         ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst3_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 0                 ; ON      ;
;      - inst93~0                                                                                                                                                                  ; 0                 ; ON      ;
;      - inst94~5                                                                                                                                                                  ; 0                 ; ON      ;
;      - inst91~0                                                                                                                                                                  ; 0                 ; ON      ;
; IN_ALTERA1                                                                                                                                                                       ;                   ;         ;
;      - busmux:inst174|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~1                                                                                                     ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                                                ; 0                 ; ON      ;
;      - AutoDAQ_SK2CMS_v1a:inst199|Mux10~1                                                                                                                                        ; 0                 ; ON      ;
; IN_ALTERA2                                                                                                                                                                       ;                   ;         ;
;      - busmux:inst118|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~0                                                                                                     ; 0                 ; ON      ;
; IN_ALTERA4                                                                                                                                                                       ;                   ;         ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst2_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 0                 ; ON      ;
; digital_probe1                                                                                                                                                                   ;                   ;         ;
;      - out_altera1                                                                                                                                                               ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 0                 ; ON      ;
; digital_probe2                                                                                                                                                                   ;                   ;         ;
;      - out_altera2                                                                                                                                                               ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 0                 ; ON      ;
; TrigOutb                                                                                                                                                                         ;                   ;         ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                                                ; 0                 ; ON      ;
;      - busmux:inst173|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~0                                                                                                     ; 0                 ; ON      ;
;      - delay_OR_trigger:inst1|lpm_shiftreg:lpm_shiftreg_component|dffs[0]                                                                                                        ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst7_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                                                ; 0                 ; ON      ;
; end_readout2                                                                                                                                                                     ;                   ;         ;
;      - busmux:inst173|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~1                                                                                                     ; 1                 ; ON      ;
;      - AutoDAQ_SK2_v1:inst130|Mux3~1                                                                                                                                             ; 1                 ; ON      ;
;      - AutoDAQ_SK2_v1:inst130|Mux13~2                                                                                                                                            ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|ERO2                                                                                                                                           ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|Hit_Memory[0]                                                                                                                                  ; 1                 ; ON      ;
; IN_ALTERA6                                                                                                                                                                       ;                   ;         ;
;      - busmux:inst173|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~0                                                                                                     ; 0                 ; ON      ;
; sr_out                                                                                                                                                                           ;                   ;         ;
;      - DAQ1                                                                                                                                                                      ; 1                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|SPY1                                                                                                                                           ; 1                 ; ON      ;
; srout_read                                                                                                                                                                       ;                   ;         ;
;      - DAQ10                                                                                                                                                                     ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|SPY4                                                                                                                                           ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|checksum_read                                                                                                                                  ; 0                 ; ON      ;
; ChipSatb                                                                                                                                                                         ;                   ;         ;
;      - AutoDAQ_SK2CMS_v1a:inst199|Mux9~0                                                                                                                                         ; 0                 ; ON      ;
;      - AutoDAQ_SK2_v1:inst130|Mux10~0                                                                                                                                            ; 0                 ; ON      ;
;      - AutoDAQ_SK2_v1:inst130|Mux11~0                                                                                                                                            ; 0                 ; ON      ;
;      - SlowControl_SK2_ERO:inst15|Sat~0                                                                                                                                          ; 0                 ; ON      ;
; clk_gene_ext                                                                                                                                                                     ;                   ;         ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                                                ; 1                 ; ON      ;
; hold_conn                                                                                                                                                                        ;                   ;         ;
;      - busmux:inst128|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                                                       ; 1                 ; ON      ;
; clk_osc                                                                                                                                                                          ;                   ;         ;
; ADC[5]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 0                 ; ON      ;
; ADC[4]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 1                 ; ON      ;
; OTR                                                                                                                                                                              ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 1                 ; ON      ;
; ADC[2]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 1                 ; ON      ;
; ADC[10]                                                                                                                                                                          ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 0                 ; ON      ;
; ADC[0]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 1                 ; ON      ;
; ADC[8]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a5 ; 0                 ; ON      ;
; ADC[1]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1 ; 0                 ; ON      ;
; ADC[9]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1            ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1 ; 1                 ; ON      ;
; ADC[3]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1 ; 0                 ; ON      ;
; ADC[11]                                                                                                                                                                          ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1 ; 0                 ; ON      ;
; ADC[7]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1            ; 0                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1 ; 0                 ; ON      ;
; ADC[6]                                                                                                                                                                           ;                   ;         ;
;      - ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1            ; 1                 ; ON      ;
;      - ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ram_block7a1 ; 1                 ; ON      ;
; TransmitOn1b                                                                                                                                                                     ;                   ;         ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 0                 ; ON      ;
; TransmitOn2b                                                                                                                                                                     ;                   ;         ;
;      - SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst5_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                                                ; 0                 ; ON      ;
; Dout2b                                                                                                                                                                           ;                   ;         ;
;      - TransmitRam:inst70|shift8register:shift8register_inst|lpm_shiftreg:lpm_shiftreg_component|dffs[0]                                                                         ; 0                 ; ON      ;
; Dout1b                                                                                                                                                                           ;                   ;         ;
;      - TransmitRam:inst70|shift8register:shift8register_inst|lpm_shiftreg:lpm_shiftreg_component|dffs[0]                                                                         ; 1                 ; ON      ;
; nTXE                                                                                                                                                                             ;                   ;         ;
;      - usb_full_interface_v:inst10|txe_r1                                                                                                                                        ; 0                 ; ON      ;
; nRXF                                                                                                                                                                             ;                   ;         ;
;      - usb_full_interface_v:inst10|rxf_r1                                                                                                                                        ; 1                 ; ON      ;
; DAQ11                                                                                                                                                                            ;                   ;         ;
; DAQ4                                                                                                                                                                             ;                   ;         ;
; USB[7]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[7]                                                                                                                 ; 1                 ; ON      ;
; USB[6]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[6]                                                                                                                 ; 0                 ; ON      ;
; USB[5]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[5]                                                                                                                 ; 1                 ; ON      ;
; USB[4]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[4]                                                                                                                 ; 0                 ; ON      ;
; USB[3]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[3]                                                                                                                 ; 1                 ; ON      ;
; USB[2]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[2]                                                                                                                 ; 1                 ; ON      ;
; USB[1]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[1]                                                                                                                 ; 0                 ; ON      ;
; USB[0]                                                                                                                                                                           ;                   ;         ;
;      - usb_full_interface_v:inst10|rxunit:m_rxunit|data_latch[0]                                                                                                                 ; 0                 ; ON      ;
; DAQ12                                                                                                                                                                            ;                   ;         ;
; DAQ9                                                                                                                                                                             ;                   ;         ;
; DAQ0                                                                                                                                                                             ;                   ;         ;
; DAQ2                                                                                                                                                                             ;                   ;         ;
; DAQ3                                                                                                                                                                             ;                   ;         ;
; DAQ5                                                                                                                                                                             ;                   ;         ;
; DAQ7                                                                                                                                                                             ;                   ;         ;
; DAQ6                                                                                                                                                                             ;                   ;         ;
; DAQ8                                                                                                                                                                             ;                   ;         ;
; DAQ1                                                                                                                                                                             ;                   ;         ;
; DAQ10                                                                                                                                                                            ;                   ;         ;
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------------+---------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Control Signals                                                                                                                                                                                                                                          ;
+------------------------------------------------------------------------------------------------------------------------------------------------+---------------+---------+----------------------------+--------+----------------------+------------------+
; Name                                                                                                                                           ; Location      ; Fan-Out ; Usage                      ; Global ; Global Resource Used ; Global Line Name ;
+------------------------------------------------------------------------------------------------------------------------------------------------+---------------+---------+----------------------------+--------+----------------------+------------------+
; ADC_AD9220_all:inst200|Mux10~0                                                                                                                 ; LC_X14_Y14_N4 ; 11      ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|Mux8~0                                                                                                                  ; LC_X19_Y14_N8 ; 10      ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|comb~0                                                                                                                  ; LC_X15_Y14_N0 ; 325     ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_fefifo_30d:read_state|llreq~0            ; LC_X16_Y13_N1 ; 18      ; Clock enable               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|valid_wreq~1                               ; LC_X11_Y16_N7 ; 18      ; Clock enable, Write enable ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|valid_rreq~0                               ; LC_X20_Y12_N7 ; 18      ; Clock enable               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|valid_wreq~0                               ; LC_X8_Y15_N6  ; 18      ; Clock enable, Write enable ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|mem_startcycle~0                                                                                                        ; LC_X19_Y14_N0 ; 2       ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|mem_startcycle~1                                                                                                        ; LC_X19_Y14_N5 ; 1       ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all:inst200|reg_8bits:reg_8bits_inst|lpm_ff:lpm_ff_component|dffs[7]                                                                ; LC_X19_Y14_N2 ; 1       ; Clock                      ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|Hit_storage~2                                                                                                       ; LC_X15_Y15_N8 ; 328     ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|Mux13~0                                                                                                             ; LC_X13_Y13_N9 ; 6       ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|Mux13~1                                                                                                             ; LC_X13_Y13_N3 ; 10      ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|Mux18~0                                                                                                             ; LC_X23_Y17_N4 ; 6       ; Clock enable               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|Mux6                                                                                                                ; LC_X14_Y13_N7 ; 5       ; Clock                      ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_fefifo_ghc:read_state|llreq~0 ; LC_X14_Y17_N8 ; 18      ; Clock enable               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|valid_wreq~1                    ; LC_X12_Y18_N1 ; 19      ; Clock enable, Write enable ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|valid_rreq~0                    ; LC_X10_Y9_N2  ; 18      ; Clock enable               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|valid_wreq~0                    ; LC_X12_Y12_N4 ; 19      ; Clock enable, Write enable ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|mem_startcycle~6                                                                                                    ; LC_X15_Y14_N5 ; 1       ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|mem_startcycle~7                                                                                                    ; LC_X15_Y14_N3 ; 5       ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|reg_8bits:reg_8bits_inst|lpm_ff:lpm_ff_component|dffs[7]                                                            ; LC_X23_Y17_N7 ; 1       ; Clock                      ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|rst_SM                                                                                                              ; LC_X15_Y14_N6 ; 5       ; Async. clear               ; no     ; --                   ; --               ;
; ADC_AD9220_all_CMS:inst182|srst_2b                                                                                                             ; LC_X13_Y13_N8 ; 2       ; Sync. clear                ; no     ; --                   ; --               ;
; AutoDAQ_SK2CMS_v1a:inst199|Mux13~0                                                                                                             ; LC_X23_Y16_N9 ; 2       ; Clock enable               ; no     ; --                   ; --               ;
; AutoDAQ_SK2CMS_v1a:inst199|Mux1~0                                                                                                              ; LC_X24_Y14_N5 ; 4       ; Async. clear               ; no     ; --                   ; --               ;
; AutoDAQ_SK2CMS_v1a:inst199|Mux4~0                                                                                                              ; LC_X25_Y11_N8 ; 27      ; Async. clear               ; no     ; --                   ; --               ;
; AutoDAQ_SK2_v1:inst130|Mux4~0                                                                                                                  ; LC_X27_Y14_N5 ; 13      ; Async. clear               ; no     ; --                   ; --               ;
; AutoDAQ_SK2_v1:inst130|StateMe[1]                                                                                                              ; LC_X28_Y14_N9 ; 15      ; Sync. clear                ; no     ; --                   ; --               ;
; AutoDAQ_SK2_v1:inst130|StateMe[3]                                                                                                              ; LC_X27_Y14_N9 ; 15      ; Sync. clear                ; no     ; --                   ; --               ;
; RSwithTimeOut:inst122|reset_RShold                                                                                                             ; LC_X26_Y9_N8  ; 6       ; Sync. clear                ; no     ; --                   ; --               ;
; RSwithTimeOut:inst122|reset_h~0                                                                                                                ; LC_X25_Y13_N7 ; 1       ; Async. clear               ; no     ; --                   ; --               ;
; Scurve_1input_16bits_sk2_cms:inst196|EnableCountT                                                                                              ; LC_X26_Y17_N1 ; 19      ; Async. clear               ; no     ; --                   ; --               ;
; Scurve_1input_16bits_sk2_cms:inst196|Reset_Int                                                                                                 ; LC_X24_Y10_N4 ; 2       ; Async. clear               ; no     ; --                   ; --               ;
; Scurve_1input_16bits_sk2_cms:inst196|aclr~0                                                                                                    ; LC_X24_Y10_N8 ; 33      ; Async. clear               ; no     ; --                   ; --               ;
; Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncTrig_2|lpm_ff:lpm_ff_component|dffs[0]                                                   ; LC_X24_Y11_N9 ; 17      ; Clock                      ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux10~0                                                                                                             ; LC_X21_Y17_N4 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux11~0                                                                                                             ; LC_X25_Y17_N5 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux13~0                                                                                                             ; LC_X25_Y17_N3 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux14~0                                                                                                             ; LC_X24_Y15_N9 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux15~2                                                                                                             ; LC_X24_Y15_N3 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux16~0                                                                                                             ; LC_X25_Y17_N6 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux5~0                                                                                                              ; LC_X16_Y11_N7 ; 4       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Mux9~1                                                                                                              ; LC_X25_Y17_N9 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Sat~0                                                                                                               ; LC_X23_Y13_N4 ; 1       ; Async. load                ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|Shift_order[0]~1                                                                                                    ; LC_X16_Y11_N2 ; 2       ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|ck_read                                                                                                             ; LC_X13_Y11_N8 ; 2       ; Clock                      ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|comb~0                                                                                                              ; LC_X16_Y11_N3 ; 4       ; Async. clear               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|valid_rreq~0                                      ; LC_X30_Y14_N2 ; 14      ; Clock enable               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|valid_wreq~0                                      ; LC_X27_Y9_N2  ; 13      ; Clock enable, Write enable ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[4]                                     ; LC_X21_Y13_N2 ; 6       ; Output enable              ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[6]                                     ; LC_X21_Y10_N5 ; 2       ; Async. clear               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[7]                                     ; LC_X22_Y18_N8 ; 1       ; Async. clear               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst1_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                     ; LC_X16_Y11_N6 ; 1       ; Clock                      ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|mem_startcycle~0                                                                                                    ; LC_X16_Y11_N4 ; 1       ; Async. clear               ; no     ; --                   ; --               ;
; SlowControl_SK2_ERO:inst15|sr_ck                                                                                                               ; LC_X15_Y11_N6 ; 3       ; Clock                      ; no     ; --                   ; --               ;
; TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_graycounter_826:rdptr_g|cntr_cout[0]~2          ; LC_X16_Y9_N2  ; 27      ; Clock enable               ; no     ; --                   ; --               ;
; TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|valid_wreq~0                                      ; LC_X16_Y7_N9  ; 26      ; Clock enable, Write enable ; no     ; --                   ; --               ;
; busmux:inst101|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X26_Y10_N8 ; 2       ; Clock                      ; no     ; --                   ; --               ;
; busmux:inst103|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X27_Y15_N9 ; 20      ; Clock                      ; no     ; --                   ; --               ;
; busmux:inst128|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X16_Y13_N2 ; 3       ; Clock                      ; no     ; --                   ; --               ;
; busmux:inst129|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X27_Y10_N7 ; 392     ; Clock                      ; yes    ; Global Clock         ; GCLK4            ;
; busmux:inst139|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X27_Y10_N9 ; 121     ; Clock                      ; yes    ; Global Clock         ; GCLK7            ;
; busmux:inst160|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X27_Y10_N0 ; 36      ; Clock                      ; yes    ; Global Clock         ; GCLK5            ;
; busmux:inst163|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; LC_X26_Y10_N0 ; 9       ; Clock                      ; no     ; --                   ; --               ;
; busmux:inst72|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~0                                                                           ; LC_X25_Y13_N8 ; 11      ; Clock enable               ; no     ; --                   ; --               ;
; busmux:inst73|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                             ; LC_X24_Y10_N5 ; 6       ; Clock                      ; no     ; --                   ; --               ;
; busmux:inst76|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                             ; LC_X25_Y13_N4 ; 23      ; Clock                      ; no     ; --                   ; --               ;
; busmux:inst96|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~2                                                                           ; LC_X24_Y14_N7 ; 7       ; Clock                      ; no     ; --                   ; --               ;
; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[2]                                                              ; LC_X27_Y10_N3 ; 675     ; Clock                      ; yes    ; Global Clock         ; GCLK6            ;
; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[3]                                                              ; LC_X27_Y10_N4 ; 81      ; Clock                      ; yes    ; Global Clock         ; GCLK1            ;
; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[4]                                                              ; LC_X27_Y10_N5 ; 7       ; Clock                      ; no     ; --                   ; --               ;
; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[5]                                                              ; LC_X27_Y10_N6 ; 8       ; Clock                      ; no     ; --                   ; --               ;
; clk_osc                                                                                                                                        ; PIN_28        ; 1       ; Clock                      ; no     ; --                   ; --               ;
; end_readout1                                                                                                                                   ; PIN_75        ; 6       ; Async. load                ; no     ; --                   ; --               ;
; end_readout2                                                                                                                                   ; PIN_76        ; 5       ; Async. load                ; no     ; --                   ; --               ;
; inst170                                                                                                                                        ; LC_X25_Y9_N4  ; 256     ; Async. clear               ; no     ; --                   ; --               ;
; inst181                                                                                                                                        ; LC_X23_Y16_N6 ; 9       ; Async. clear               ; no     ; --                   ; --               ;
; inst183                                                                                                                                        ; LC_X22_Y17_N1 ; 18      ; Async. clear               ; no     ; --                   ; --               ;
; inst198                                                                                                                                        ; LC_X27_Y10_N8 ; 6       ; Clock                      ; no     ; --                   ; --               ;
; inst218                                                                                                                                        ; LC_X26_Y11_N6 ; 12      ; Async. clear               ; no     ; --                   ; --               ;
; inst28                                                                                                                                         ; LC_X19_Y13_N5 ; 2       ; Clock                      ; no     ; --                   ; --               ;
; inst51                                                                                                                                         ; LC_X24_Y15_N4 ; 4       ; Async. clear               ; no     ; --                   ; --               ;
; inst77                                                                                                                                         ; LC_X24_Y14_N2 ; 225     ; Async. clear               ; no     ; --                   ; --               ;
; pll_sk2:inst|altpll:altpll_component|_clk0                                                                                                     ; PLL_1         ; 6       ; Clock                      ; yes    ; Global Clock         ; GCLK2            ;
; pll_sk2:inst|altpll:altpll_component|_clk1                                                                                                     ; PLL_1         ; 259     ; Clock                      ; yes    ; Global Clock         ; GCLK0            ;
; pwr_reset                                                                                                                                      ; PIN_121       ; 464     ; Async. clear               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux0~0                                                                                                           ; LC_X24_Y16_N6 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux1~0                                                                                                           ; LC_X20_Y14_N1 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux2~0                                                                                                           ; LC_X20_Y14_N3 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux3~0                                                                                                           ; LC_X24_Y16_N8 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux4~0                                                                                                           ; LC_X25_Y12_N9 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux5~1                                                                                                           ; LC_X25_Y12_N7 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux6~0                                                                                                           ; LC_X23_Y16_N4 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; static_8bit_registers:inst124|Mux7~0                                                                                                           ; LC_X23_Y16_N2 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|always2~1                                                                                                          ; LC_X34_Y19_N2 ; 8       ; Output enable              ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|interruptunit:m_interruptunit|status_byte[3]~12                                                                    ; LC_X21_Y16_N6 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|readrequnit:m_readrequnit|rdreq_presentstate.10                                                                    ; LC_X23_Y10_N8 ; 11      ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|Equal3~5                                                                                           ; LC_X10_Y14_N6 ; 10      ; Sync. clear                ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|always8~0                                                                                          ; LC_X19_Y19_N3 ; 8       ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|n_write                                                                                            ; LC_X8_Y10_N2  ; 129     ; Clock, Clock enable        ; yes    ; Global Clock         ; GCLK3            ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0101                                                                               ; LC_X15_Y17_N4 ; 10      ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.0111                                                                               ; LC_X15_Y17_N2 ; 11      ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|rx_presentstate.1011                                                                               ; LC_X15_Y17_N7 ; 10      ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|txunit:m_txunit|always8~0                                                                                          ; LC_X21_Y18_N1 ; 17      ; Sync. clear                ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[4]~34                                                                                     ; LC_X21_Y18_N7 ; 17      ; Clock enable               ; no     ; --                   ; --               ;
; usb_full_interface_v:inst10|txunit:m_txunit|tx_presentstate.10011                                                                              ; LC_X21_Y18_N4 ; 11      ; Clock enable               ; no     ; --                   ; --               ;
+------------------------------------------------------------------------------------------------------------------------------------------------+---------------+---------+----------------------------+--------+----------------------+------------------+


+-------------------------------------------------------------------------------------------------------------------------------------------------------+
; Global & Other Fast Signals                                                                                                                           ;
+-----------------------------------------------------------------------------------+---------------+---------+----------------------+------------------+
; Name                                                                              ; Location      ; Fan-Out ; Global Resource Used ; Global Line Name ;
+-----------------------------------------------------------------------------------+---------------+---------+----------------------+------------------+
; busmux:inst129|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]               ; LC_X27_Y10_N7 ; 392     ; Global Clock         ; GCLK4            ;
; busmux:inst139|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]               ; LC_X27_Y10_N9 ; 121     ; Global Clock         ; GCLK7            ;
; busmux:inst160|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]               ; LC_X27_Y10_N0 ; 36      ; Global Clock         ; GCLK5            ;
; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[2] ; LC_X27_Y10_N3 ; 675     ; Global Clock         ; GCLK6            ;
; clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[3] ; LC_X27_Y10_N4 ; 81      ; Global Clock         ; GCLK1            ;
; pll_sk2:inst|altpll:altpll_component|_clk0                                        ; PLL_1         ; 6       ; Global Clock         ; GCLK2            ;
; pll_sk2:inst|altpll:altpll_component|_clk1                                        ; PLL_1         ; 259     ; Global Clock         ; GCLK0            ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|n_write                               ; LC_X8_Y10_N2  ; 129     ; Global Clock         ; GCLK3            ;
+-----------------------------------------------------------------------------------+---------------+---------+----------------------+------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------+
; Non-Global High Fan-Out Signals                                                                                                                          ;
+------------------------------------------------------------------------------------------------------------------------------------------------+---------+
; Name                                                                                                                                           ; Fan-Out ;
+------------------------------------------------------------------------------------------------------------------------------------------------+---------+
; pwr_reset                                                                                                                                      ; 465     ;
; ADC_AD9220_all_CMS:inst182|Hit_storage~2                                                                                                       ; 328     ;
; ADC_AD9220_all:inst200|comb~0                                                                                                                  ; 325     ;
; inst170                                                                                                                                        ; 256     ;
; inst77                                                                                                                                         ; 225     ;
; static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[0]                                  ; 125     ;
; static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[1]                                  ; 82      ;
; SlowControl_SK2_ERO:inst15|latch_8:Ins0_7_Latch8|reg_8bits:inst6_reg_8bits|lpm_ff:lpm_ff_component|dffs[5]                                     ; 46      ;
; static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[2]                                  ; 35      ;
; usb_full_interface_v:inst10|subaddtotx[3]~1                                                                                                    ; 35      ;
; TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|valid_wreq~0                                      ; 34      ;
; Scurve_1input_16bits_sk2_cms:inst196|aclr~0                                                                                                    ; 33      ;
; static_8bit_registers:inst124|latch_8:Ins0_7_Latch8|reg_8bits:inst0_reg_8bits|lpm_ff:lpm_ff_component|dffs[3]                                  ; 31      ;
; TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|a_graycounter_826:rdptr_g|cntr_cout[0]~2          ; 27      ;
; AutoDAQ_SK2CMS_v1a:inst199|Mux4~0                                                                                                              ; 27      ;
; usb_full_interface_v:inst10|n_read~0                                                                                                           ; 25      ;
; busmux:inst76|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                             ; 24      ;
; usb_full_interface_v:inst10|txunit:m_txunit|txe_latch                                                                                          ; 23      ;
; Firmware_v:inst14|Read_Word:Read_Word0|User_Data[7]~87                                                                                         ; 22      ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|valid_wreq~0                    ; 21      ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|valid_wreq~1                    ; 21      ;
; busmux:inst103|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]                                                                            ; 20      ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|valid_wreq~1                               ; 20      ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|valid_wreq~0                               ; 20      ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|runtx                                                                                              ; 20      ;
; usb_full_interface_v:inst10|subaddtotx[2]~3                                                                                                    ; 20      ;
; Scurve_1input_16bits_sk2_cms:inst196|EnableCountT                                                                                              ; 19      ;
; Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:Sync2|lpm_ff:lpm_ff_component|dffs[0]                                                        ; 19      ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|valid_rreq~0                    ; 18      ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|a_fefifo_ghc:read_state|llreq~0 ; 18      ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|a_fefifo_30d:read_state|llreq~0            ; 18      ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|valid_rreq~0                               ; 18      ;
; Firmware_v:inst14|Read_Word:Read_Word0|User_Data[6]~106                                                                                        ; 18      ;
; ADC_AD9220_all_CMS:inst182|Read_Word:Read_Word2|User_Data[3]~37                                                                                ; 18      ;
; SlowControl_SK2_ERO:inst15|Read_Word:Read_Word4|User_Data[1]~20                                                                                ; 18      ;
; Firmware_v:inst14|Read_Word:Read_Word0|User_Data[0]~68                                                                                         ; 18      ;
; ADC_AD9220_all_CMS:inst182|Read_Word:Read_Word2|User_Data[2]~19                                                                                ; 18      ;
; Firmware_v:inst14|Read_Word:Read_Word0|User_Data[4]~49                                                                                         ; 18      ;
; Firmware_v:inst14|Read_Word:Read_Word0|User_Data[5]~31                                                                                         ; 18      ;
; inst183                                                                                                                                        ; 18      ;
; usb_full_interface_v:inst10|txunit:m_txunit|cptNdata[4]~34                                                                                     ; 17      ;
; usb_full_interface_v:inst10|txunit:m_txunit|always8~0                                                                                          ; 17      ;
; Scurve_1input_16bits_sk2_cms:inst196|flipflopaclr:SyncTrig_2|lpm_ff:lpm_ff_component|dffs[0]                                                   ; 17      ;
; usb_full_interface_v:inst10|readrequnit:m_readrequnit|busyreadreq                                                                              ; 17      ;
; ADC_AD9220_all_CMS:inst182|StateMachine[0]                                                                                                     ; 17      ;
; usb_full_interface_v:inst10|rxunit:m_rxunit|rxf_latch                                                                                          ; 16      ;
; SlowControl_SK2_ERO:inst15|Equal0~0                                                                                                            ; 16      ;
; static_8bit_registers:inst124|Read_Word:Read_Word7|User_Data[7]~0                                                                              ; 16      ;
; usb_full_interface_v:inst10|subaddtotx[4]~0                                                                                                    ; 16      ;
; ADC_AD9220_all_CMS:inst182|StateMachine[1]                                                                                                     ; 16      ;
+------------------------------------------------------------------------------------------------------------------------------------------------+---------+


+---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter RAM Summary                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+------+------------------+-------------+--------------+--------------+--------------+--------------+------------------------+-------------------------+------------------------+-------------------------+-------+-----------------------------+-----------------------------+-----------------------------+-----------------------------+---------------------+------+------+-------------------------------------------------------------------------------------------------+
; Name                                                                                                                                                                    ; Type ; Mode             ; Clock Mode  ; Port A Depth ; Port A Width ; Port B Depth ; Port B Width ; Port A Input Registers ; Port A Output Registers ; Port B Input Registers ; Port B Output Registers ; Size  ; Implementation Port A Depth ; Implementation Port A Width ; Implementation Port B Depth ; Implementation Port B Width ; Implementation Bits ; M4Ks ; MIF  ; Location                                                                                        ;
+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+------+------------------+-------------+--------------+--------------+--------------+--------------+------------------------+-------------------------+------------------------+-------------------------+-------+-----------------------------+-----------------------------+-----------------------------+-----------------------------+---------------------+------+------+-------------------------------------------------------------------------------------------------+
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ALTSYNCRAM            ; AUTO ; Simple Dual Port ; Dual Clocks ; 1024         ; 8            ; 1024         ; 8            ; yes                    ; no                      ; yes                    ; no                      ; 8192  ; 1024                        ; 8                           ; 1024                        ; 8                           ; 8192                ; 2    ; None ; M4K_X17_Y16, M4K_X17_Y17                                                                        ;
; ADC_AD9220_all:inst200|fifo_adc:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_pdi1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ALTSYNCRAM            ; AUTO ; Simple Dual Port ; Dual Clocks ; 1024         ; 8            ; 1024         ; 8            ; yes                    ; no                      ; yes                    ; no                      ; 8192  ; 1024                        ; 8                           ; 1024                        ; 8                           ; 8192                ; 2    ; None ; M4K_X17_Y14, M4K_X17_Y15                                                                        ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_20|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ALTSYNCRAM ; AUTO ; Simple Dual Port ; Dual Clocks ; 1024         ; 8            ; 1024         ; 8            ; yes                    ; no                      ; yes                    ; no                      ; 8192  ; 1024                        ; 8                           ; 1024                        ; 8                           ; 8192                ; 2    ; None ; M4K_X17_Y18, M4K_X17_Y19                                                                        ;
; ADC_AD9220_all_CMS:inst182|fifo_acd_SK2CMS:fifo_adc_inst_21|dcfifo:dcfifo_component|dcfifo_elh1:auto_generated|dpram_n3v:fiforam|altsyncram_pof1:altsyncram6|ALTSYNCRAM ; AUTO ; Simple Dual Port ; Dual Clocks ; 1024         ; 8            ; 1024         ; 8            ; yes                    ; no                      ; yes                    ; no                      ; 8192  ; 1024                        ; 8                           ; 1024                        ; 8                           ; 8192                ; 2    ; None ; M4K_X17_Y11, M4K_X17_Y12                                                                        ;
; SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dpram_e2v:fiforam|altsyncram_7mf1:altsyncram6|ALTSYNCRAM                   ; AUTO ; Simple Dual Port ; Dual Clocks ; 256          ; 8            ; 256          ; 8            ; yes                    ; no                      ; yes                    ; no                      ; 2048  ; 256                         ; 8                           ; 256                         ; 8                           ; 2048                ; 1    ; None ; M4K_X17_Y13                                                                                     ;
; TransmitRam:inst70|big_fifo:big_fifo_inst|dcfifo:dcfifo_component|dcfifo_9ei1:auto_generated|dpram_p3v:fiforam|altsyncram_tof1:altsyncram6|ALTSYNCRAM                   ; AUTO ; Simple Dual Port ; Dual Clocks ; 4096         ; 8            ; 4096         ; 8            ; yes                    ; no                      ; yes                    ; no                      ; 32768 ; 4096                        ; 8                           ; 4096                        ; 8                           ; 32768               ; 8    ; None ; M4K_X17_Y5, M4K_X17_Y3, M4K_X17_Y6, M4K_X17_Y10, M4K_X17_Y9, M4K_X17_Y8, M4K_X17_Y7, M4K_X17_Y4 ;
+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+------+------------------+-------------+--------------+--------------+--------------+--------------+------------------------+-------------------------+------------------------+-------------------------+-------+-----------------------------+-----------------------------+-----------------------------+-----------------------------+---------------------+------+------+-------------------------------------------------------------------------------------------------+
Note: Fitter may spread logical memories into multiple blocks to improve timing. The actual required RAM blocks can be found in the Fitter Resource Usage section.


+------------------------------------------------------+
; Interconnect Usage Summary                           ;
+----------------------------+-------------------------+
; Interconnect Resource Type ; Usage                   ;
+----------------------------+-------------------------+
; C4s                        ; 2,473 / 16,320 ( 15 % ) ;
; Direct links               ; 507 / 21,944 ( 2 % )    ;
; Global clocks              ; 8 / 8 ( 100 % )         ;
; LAB clocks                 ; 100 / 240 ( 42 % )      ;
; LUT chains                 ; 101 / 5,382 ( 2 % )     ;
; Local interconnects        ; 3,635 / 21,944 ( 17 % ) ;
; M4K buffers                ; 48 / 720 ( 7 % )        ;
; R4s                        ; 2,641 / 14,640 ( 18 % ) ;
+----------------------------+-------------------------+


+----------------------------------------------------------------------------+
; LAB Logic Elements                                                         ;
+--------------------------------------------+-------------------------------+
; Number of Logic Elements  (Average = 8.47) ; Number of LABs  (Total = 287) ;
+--------------------------------------------+-------------------------------+
; 1                                          ; 6                             ;
; 2                                          ; 6                             ;
; 3                                          ; 7                             ;
; 4                                          ; 5                             ;
; 5                                          ; 11                            ;
; 6                                          ; 12                            ;
; 7                                          ; 19                            ;
; 8                                          ; 28                            ;
; 9                                          ; 42                            ;
; 10                                         ; 151                           ;
+--------------------------------------------+-------------------------------+


+--------------------------------------------------------------------+
; LAB-wide Signals                                                   ;
+------------------------------------+-------------------------------+
; LAB-wide Signals  (Average = 2.16) ; Number of LABs  (Total = 287) ;
+------------------------------------+-------------------------------+
; 1 Async. clear                     ; 247                           ;
; 1 Async. load                      ; 2                             ;
; 1 Clock                            ; 223                           ;
; 1 Clock enable                     ; 49                            ;
; 1 Sync. clear                      ; 4                             ;
; 2 Async. clears                    ; 19                            ;
; 2 Clock enables                    ; 28                            ;
; 2 Clocks                           ; 47                            ;
+------------------------------------+-------------------------------+


+-----------------------------------------------------------------------------+
; LAB Signals Sourced                                                         ;
+---------------------------------------------+-------------------------------+
; Number of Signals Sourced  (Average = 9.20) ; Number of LABs  (Total = 287) ;
+---------------------------------------------+-------------------------------+
; 0                                           ; 0                             ;
; 1                                           ; 6                             ;
; 2                                           ; 6                             ;
; 3                                           ; 5                             ;
; 4                                           ; 6                             ;
; 5                                           ; 7                             ;
; 6                                           ; 9                             ;
; 7                                           ; 9                             ;
; 8                                           ; 29                            ;
; 9                                           ; 31                            ;
; 10                                          ; 124                           ;
; 11                                          ; 20                            ;
; 12                                          ; 15                            ;
; 13                                          ; 8                             ;
; 14                                          ; 9                             ;
; 15                                          ; 1                             ;
; 16                                          ; 1                             ;
; 17                                          ; 0                             ;
; 18                                          ; 1                             ;
+---------------------------------------------+-------------------------------+


+---------------------------------------------------------------------------------+
; LAB Signals Sourced Out                                                         ;
+-------------------------------------------------+-------------------------------+
; Number of Signals Sourced Out  (Average = 5.82) ; Number of LABs  (Total = 287) ;
+-------------------------------------------------+-------------------------------+
; 0                                               ; 0                             ;
; 1                                               ; 18                            ;
; 2                                               ; 20                            ;
; 3                                               ; 28                            ;
; 4                                               ; 41                            ;
; 5                                               ; 35                            ;
; 6                                               ; 31                            ;
; 7                                               ; 31                            ;
; 8                                               ; 25                            ;
; 9                                               ; 13                            ;
; 10                                              ; 35                            ;
; 11                                              ; 7                             ;
; 12                                              ; 2                             ;
; 13                                              ; 0                             ;
; 14                                              ; 0                             ;
; 15                                              ; 0                             ;
; 16                                              ; 0                             ;
; 17                                              ; 0                             ;
; 18                                              ; 1                             ;
+-------------------------------------------------+-------------------------------+


+------------------------------------------------------------------------------+
; LAB Distinct Inputs                                                          ;
+----------------------------------------------+-------------------------------+
; Number of Distinct Inputs  (Average = 10.63) ; Number of LABs  (Total = 287) ;
+----------------------------------------------+-------------------------------+
; 0                                            ; 0                             ;
; 1                                            ; 0                             ;
; 2                                            ; 1                             ;
; 3                                            ; 24                            ;
; 4                                            ; 9                             ;
; 5                                            ; 19                            ;
; 6                                            ; 40                            ;
; 7                                            ; 30                            ;
; 8                                            ; 18                            ;
; 9                                            ; 11                            ;
; 10                                           ; 14                            ;
; 11                                           ; 10                            ;
; 12                                           ; 10                            ;
; 13                                           ; 11                            ;
; 14                                           ; 13                            ;
; 15                                           ; 4                             ;
; 16                                           ; 5                             ;
; 17                                           ; 10                            ;
; 18                                           ; 8                             ;
; 19                                           ; 12                            ;
; 20                                           ; 9                             ;
; 21                                           ; 20                            ;
; 22                                           ; 8                             ;
+----------------------------------------------+-------------------------------+


+--------------------------------------------------------------------+
; Fitter Device Options                                              ;
+----------------------------------------------+---------------------+
; Option                                       ; Setting             ;
+----------------------------------------------+---------------------+
; Enable user-supplied start-up clock (CLKUSR) ; Off                 ;
; Enable device-wide reset (DEV_CLRn)          ; Off                 ;
; Enable device-wide output enable (DEV_OE)    ; Off                 ;
; Enable INIT_DONE output                      ; Off                 ;
; Configuration scheme                         ; Active Serial       ;
; Error detection CRC                          ; Off                 ;
; ASDO,nCSO                                    ; As input tri-stated ;
; Reserve all unused pins                      ; As input tri-stated ;
; Base pin-out file on sameframe device        ; Off                 ;
+----------------------------------------------+---------------------+


+-------------------------------------------------------------------------------------------------------------+
; Estimated Delay Added for Hold Timing                                                                       ;
+--------------------------------------------+--------------------------------------------+-------------------+
; Source Clock(s)                            ; Destination Clock(s)                       ; Delay Added in ns ;
+--------------------------------------------+--------------------------------------------+-------------------+
; pll_sk2:inst|altpll:altpll_component|_clk0 ; pll_sk2:inst|altpll:altpll_component|_clk0 ; 221.635           ;
+--------------------------------------------+--------------------------------------------+-------------------+
Note: For more information on problematic transfers, consider running the Fitter again with the Optimize hold timing option (Settings Menu) turned off.
This will disable optimization of problematic paths and expose them for further analysis using either the TimeQuest Timing Analyzer or the Classic Timing Analyzer.


+-----------------+
; Fitter Messages ;
+-----------------+
Info: *******************************************************************
Info: Running Quartus II Fitter
    Info: Version 9.1 Build 350 03/24/2010 Service Pack 2 SJ Web Edition
    Info: Processing started: Mon Apr 30 15:17:16 2018
Info: Command: quartus_fit --read_settings_files=off --write_settings_files=off Skiroc2 -c Skiroc2
Info: Parallel compilation is enabled and will use 2 of the 2 processors detected
Info: Selected device EP1C6Q240C6 for design "Skiroc2"
Info: Implementing parameter values for PLL "pll_sk2:inst|altpll:altpll_component|pll"
    Info: Implementing clock multiplication of 4, clock division of 1, and phase shift of 0 degrees (0 ps) for pll_sk2:inst|altpll:altpll_component|_clk0 port
    Info: Implementing clock multiplication of 10, clock division of 1, and phase shift of 0 degrees (0 ps) for pll_sk2:inst|altpll:altpll_component|_clk1 port
Info: Fitter is performing an Auto Fit compilation, which may decrease Fitter effort to reduce compilation time
Info: Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices
    Info: Device EP1C12Q240C6 is compatible
Info: Fitter converted 2 user pins into dedicated programming pins
    Info: Pin ~nCSO~ is reserved at location 24
    Info: Pin ~ASDO~ is reserved at location 37
Info: Completed LVDS Placement Operation Initializations
Info: Timing-driven compilation is using the Classic Timing Analyzer
Info: Detected fmax, tsu, tco, and/or tpd requirements -- optimizing circuit to achieve only the specified requirements
Info: Completed User Assigned Global Signals Promotion Operation
Info: DQS I/O pins require 0 global routing resources
Info: Completed Regular LVDS Placement Operation
Info: Promoted PLL clock signals
    Info: Promoted signal "pll_sk2:inst|altpll:altpll_component|_clk1" to use global clock (user assigned)
    Info: Promoted signal "pll_sk2:inst|altpll:altpll_component|_clk0" to use global clock (user assigned)
Info: Completed PLL Placement Operation
Info: Automatically promoted some destinations of signal "clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[2]" to use Global clock
    Info: Destination "clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella2" may be non-global or may not use global clock
Info: Automatically promoted signal "busmux:inst129|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]" to use Global clock
Info: Automatically promoted some destinations of signal "usb_full_interface_v:inst10|rxunit:m_rxunit|n_write" to use Global clock
    Info: Destination "SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_instmemsr|lpm_ff:lpm_ff_component|dffs[0]" may be non-global or may not use global clock
    Info: Destination "SlowControl_SK2_ERO:inst15|flipflopaclr_en:flipflopaclr_en_instmemread|lpm_ff:lpm_ff_component|dffs[0]" may be non-global or may not use global clock
    Info: Destination "usb_full_interface_v:inst10|n_write_r" may be non-global or may not use global clock
    Info: Destination "usb_full_interface_v:inst10|always2~0" may be non-global or may not use global clock
    Info: Destination "SlowControl_SK2_ERO:inst15|flipflopaclr:flipflopaclr_instwr|lpm_ff:lpm_ff_component|dffs[0]" may be non-global or may not use global clock
    Info: Destination "usb_full_interface_v:inst10|rxunit:m_rxunit|always13~0" may be non-global or may not use global clock
Info: Automatically promoted signal "busmux:inst139|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]" to use Global clock
Info: Automatically promoted some destinations of signal "clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|safe_q[3]" to use Global clock
    Info: Destination "clk_div:inst2|lpm_counter:lpm_counter_component|cntr_crh:auto_generated|counter_cella3" may be non-global or may not use global clock
Info: Automatically promoted some destinations of signal "busmux:inst160|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]" to use Global clock
    Info: Destination "40M" may be non-global or may not use global clock
    Info: Destination "inst16" may be non-global or may not use global clock
Info: Completed Auto Global Promotion Operation
Info: Completed Flexible LVDS Placement Operation
Info: Starting register packing
Info: Fitter is using Normal packing mode for logic elements with Auto setting for Auto Packed Registers logic option
Info: Finished moving registers into I/O cells, LUTs, and RAM blocks
Info: Finished register packing
Info: Design uses memory blocks. Violating setup or hold times of memory block address registers for either read or write operations could cause memory contents to be corrupted. Make sure that all memory block address registers meet the setup and hold time requirements.
Info: Fitter preparation operations ending: elapsed time is 00:00:01
Info: Fitter placement preparation operations beginning
Info: Fitter placement preparation operations ending: elapsed time is 00:00:03
Info: Fitter placement operations beginning
Info: Fitter placement was successful
Info: Fitter placement operations ending: elapsed time is 00:00:08
Info: Estimated most critical path is register to memory delay of 7.704 ns
    Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LAB_X24_Y14; Fanout = 12; REG Node = 'AutoDAQ_SK2CMS_v1a:inst199|StateMe[3]'
    Info: 2: + IC(0.473 ns) + CELL(0.088 ns) = 0.561 ns; Loc. = LAB_X24_Y14; Fanout = 2; COMB Node = 'busmux:inst150|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~0'
    Info: 3: + IC(0.162 ns) + CELL(0.340 ns) = 1.063 ns; Loc. = LAB_X24_Y14; Fanout = 1; COMB Node = 'busmux:inst97|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~0'
    Info: 4: + IC(0.048 ns) + CELL(0.454 ns) = 1.565 ns; Loc. = LAB_X24_Y14; Fanout = 2; COMB Node = 'busmux:inst97|lpm_mux:$00000|mux_3fc:auto_generated|result_node[0]~2'
    Info: 5: + IC(0.414 ns) + CELL(0.088 ns) = 2.067 ns; Loc. = LAB_X24_Y14; Fanout = 225; COMB Node = 'inst77'
    Info: 6: + IC(1.201 ns) + CELL(0.088 ns) = 3.356 ns; Loc. = LAB_X21_Y12; Fanout = 9; COMB Node = 'Scurve_1input_16bits_sk2_cms:inst196|Read_Word:Read_Word18|User_Data[7]~0'
    Info: 7: + IC(0.949 ns) + CELL(0.088 ns) = 4.393 ns; Loc. = LAB_X22_Y14; Fanout = 1; COMB Node = 'Firmware_v:inst14|Read_Word:Read_Word0|User_Data[0]~60'
    Info: 8: + IC(0.583 ns) + CELL(0.454 ns) = 5.430 ns; Loc. = LAB_X23_Y12; Fanout = 2; COMB Node = 'Firmware_v:inst14|Read_Word:Read_Word0|User_Data[0]~67'
    Info: 9: + IC(0.277 ns) + CELL(0.225 ns) = 5.932 ns; Loc. = LAB_X23_Y12; Fanout = 18; COMB Node = 'Firmware_v:inst14|Read_Word:Read_Word0|User_Data[0]~68'
    Info: 10: + IC(1.498 ns) + CELL(0.274 ns) = 7.704 ns; Loc. = M4K_X17_Y13; Fanout = 1; MEM Node = 'SlowControl_SK2_ERO:inst15|fifo:fifo_inst|dcfifo:dcfifo_component|dcfifo_gai1:auto_generated|dpram_e2v:fiforam|altsyncram_7mf1:altsyncram6|ram_block7a0~porta_datain_reg0'
    Info: Total cell delay = 2.099 ns ( 27.25 % )
    Info: Total interconnect delay = 5.605 ns ( 72.75 % )
Info: Fitter routing operations beginning
Info: 49 (of 7499) connections in the design require a large routing delay to satisfy hold requirements. Refer to the Fitter report for a summary of the relevant clock transfers. Also, check the circuit's timing constraints and clocking methodology, especially multicycles and gated clocks.
Info: Average interconnect usage is 15% of the available device resources
    Info: Peak interconnect usage is 39% of the available device resources in the region that extends from location X12_Y11 to location X23_Y21
Info: Fitter routing operations ending: elapsed time is 00:00:05
Info: The Fitter performed an Auto Fit compilation.  Optimizations were skipped to reduce compilation time.
    Info: Optimizations that may affect the design's routability were skipped
Info: Completed Fixed Delay Chain Operation
Info: Started post-fitting delay annotation
Info: Delay annotation completed successfully
Info: Completed Auto Delay Chain Operation
Info: Design uses memory blocks. Violating setup or hold times of memory block address registers for either read or write operations could cause memory contents to be corrupted. Make sure that all memory block address registers meet the setup and hold time requirements.
Warning: Following 13 pins have no output enable or a GND or VCC output enable - later changes to this connectivity may change fitting results
    Info: Pin DAQ11 has a permanently enabled output enable
    Info: Pin DAQ4 has a permanently enabled output enable
    Info: Pin DAQ12 has a permanently enabled output enable
    Info: Pin DAQ9 has a permanently enabled output enable
    Info: Pin DAQ0 has a permanently enabled output enable
    Info: Pin DAQ2 has a permanently enabled output enable
    Info: Pin DAQ3 has a permanently enabled output enable
    Info: Pin DAQ5 has a permanently enabled output enable
    Info: Pin DAQ7 has a permanently enabled output enable
    Info: Pin DAQ6 has a permanently enabled output enable
    Info: Pin DAQ8 has a permanently enabled output enable
    Info: Pin DAQ1 has a permanently enabled output enable
    Info: Pin DAQ10 has a permanently enabled output enable
Info: Generated suppressed messages file D:/synchro_portable/Data/ASIC/skiroc2/firmware/Skiroc2.fit.smsg
Info: Quartus II Fitter was successful. 0 errors, 1 warning
    Info: Peak virtual memory: 259 megabytes
    Info: Processing ended: Mon Apr 30 15:17:38 2018
    Info: Elapsed time: 00:00:22
    Info: Total CPU time (on all processors): 00:00:27


+----------------------------+
; Fitter Suppressed Messages ;
+----------------------------+
The suppressed messages can be found in D:/synchro_portable/Data/ASIC/skiroc2/firmware/Skiroc2.fit.smsg.


