/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 64 64 240 320)
	(text "ADC_AD9220_all" (rect 5 0 89 12)(font "Arial" ))
	(text "inst" (rect 8 240 25 252)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "n_reset" (rect 0 0 36 12)(font "Arial" ))
		(text "n_reset" (rect 21 27 57 39)(font "Arial" ))
		(line (pt 0 32)(pt 16 32)(line_width 1))
	)
	(port
		(pt 0 48)
		(input)
		(text "n_write" (rect 0 0 34 12)(font "Arial" ))
		(text "n_write" (rect 21 43 55 55)(font "Arial" ))
		(line (pt 0 48)(pt 16 48)(line_width 1))
	)
	(port
		(pt 0 64)
		(input)
		(text "n_read" (rect 0 0 33 12)(font "Arial" ))
		(text "n_read" (rect 21 59 54 71)(font "Arial" ))
		(line (pt 0 64)(pt 16 64)(line_width 1))
	)
	(port
		(pt 0 80)
		(input)
		(text "Hold" (rect 0 0 22 12)(font "Arial" ))
		(text "Hold" (rect 21 75 43 87)(font "Arial" ))
		(line (pt 0 80)(pt 16 80)(line_width 1))
	)
	(port
		(pt 0 96)
		(input)
		(text "clock_machine" (rect 0 0 73 12)(font "Arial" ))
		(text "clock_machine" (rect 21 91 94 103)(font "Arial" ))
		(line (pt 0 96)(pt 16 96)(line_width 1))
	)
	(port
		(pt 0 112)
		(input)
		(text "subadd[6..0]" (rect 0 0 61 12)(font "Arial" ))
		(text "subadd[6..0]" (rect 21 107 82 119)(font "Arial" ))
		(line (pt 0 112)(pt 16 112)(line_width 3))
	)
	(port
		(pt 0 128)
		(input)
		(text "adc[12..1]" (rect 0 0 49 12)(font "Arial" ))
		(text "adc[12..1]" (rect 21 123 70 135)(font "Arial" ))
		(line (pt 0 128)(pt 16 128)(line_width 3))
	)
	(port
		(pt 0 144)
		(input)
		(text "OTR" (rect 0 0 22 12)(font "Arial" ))
		(text "OTR" (rect 21 139 43 151)(font "Arial" ))
		(line (pt 0 144)(pt 16 144)(line_width 1))
	)
	(port
		(pt 0 160)
		(input)
		(text "nb_channels[1..0]" (rect 0 0 87 12)(font "Arial" ))
		(text "nb_channels[1..0]" (rect 21 155 108 167)(font "Arial" ))
		(line (pt 0 160)(pt 16 160)(line_width 3))
	)
	(port
		(pt 0 192)
		(input)
		(text "nb_acq[7..0]" (rect 0 0 61 12)(font "Arial" ))
		(text "nb_acq[7..0]" (rect 21 187 82 199)(font "Arial" ))
		(line (pt 0 192)(pt 16 192)(line_width 3))
	)
	(port
		(pt 0 176)
		(input)
		(text "ck_usb" (rect 0 0 35 12)(font "Arial" ))
		(text "ck_usb" (rect 21 171 56 183)(font "Arial" ))
		(line (pt 0 176)(pt 16 176)(line_width 1))
	)
	(port
		(pt 176 48)
		(output)
		(text "clk_adc" (rect -40 0 -3 12)(font "Arial" ))
		(text "clk_adc" (rect 118 43 155 55)(font "Arial" ))
		(line (pt 176 48)(pt 160 48)(line_width 1))
	)
	(port
		(pt 176 64)
		(output)
		(text "srin_read" (rect -40 0 4 12)(font "Arial" ))
		(text "srin_read" (rect 111 59 155 71)(font "Arial" ))
		(line (pt 176 64)(pt 160 64)(line_width 1))
	)
	(port
		(pt 176 80)
		(output)
		(text "ck_read" (rect -40 0 -2 12)(font "Arial" ))
		(text "ck_read" (rect 117 75 155 87)(font "Arial" ))
		(line (pt 176 80)(pt 160 80)(line_width 1))
	)
	(port
		(pt 176 96)
		(output)
		(text "resetb_read" (rect -40 0 17 12)(font "Arial" ))
		(text "resetb_read" (rect 98 91 155 103)(font "Arial" ))
		(line (pt 176 96)(pt 160 96)(line_width 1))
	)
	(port
		(pt 176 112)
		(output)
		(text "sel_read" (rect -40 0 1 12)(font "Arial" ))
		(text "sel_read" (rect 114 107 155 119)(font "Arial" ))
		(line (pt 176 112)(pt 160 112)(line_width 1))
	)
	(port
		(pt 176 224)
		(output)
		(text "RazChn" (rect -40 0 -2 12)(font "Arial" ))
		(text "RazChn" (rect 112 216 150 228)(font "Arial" ))
		(line (pt 176 224)(pt 160 224)(line_width 1))
	)
	(port
		(pt 176 128)
		(output)
		(text "SPY1" (rect -40 0 -12 12)(font "Arial" ))
		(text "SPY1" (rect 120 120 148 132)(font "Arial" ))
		(line (pt 176 128)(pt 160 128)(line_width 1))
	)
	(port
		(pt 176 144)
		(output)
		(text "SPY2" (rect -40 0 -12 12)(font "Arial" ))
		(text "SPY2" (rect 120 136 148 148)(font "Arial" ))
		(line (pt 176 144)(pt 160 144)(line_width 1))
	)
	(port
		(pt 176 160)
		(output)
		(text "SPY3" (rect -40 0 -12 12)(font "Arial" ))
		(text "SPY3" (rect 120 152 148 164)(font "Arial" ))
		(line (pt 176 160)(pt 160 160)(line_width 1))
	)
	(port
		(pt 176 176)
		(output)
		(text "SPY4" (rect -40 0 -12 12)(font "Arial" ))
		(text "SPY4" (rect 120 168 148 180)(font "Arial" ))
		(line (pt 176 176)(pt 160 176)(line_width 1))
	)
	(port
		(pt 176 192)
		(output)
		(text "SPY5" (rect -40 0 -12 12)(font "Arial" ))
		(text "SPY5" (rect 120 184 148 196)(font "Arial" ))
		(line (pt 176 192)(pt 160 192)(line_width 1))
	)
	(port
		(pt 176 208)
		(output)
		(text "SPY6" (rect -40 0 -12 12)(font "Arial" ))
		(text "SPY6" (rect 120 200 148 212)(font "Arial" ))
		(line (pt 176 208)(pt 160 208)(line_width 1))
	)
	(port
		(pt 176 32)
		(bidir)
		(text "user_data[7..0]" (rect -40 0 34 12)(font "Arial" ))
		(text "user_data[7..0]" (rect 81 27 155 39)(font "Arial" ))
		(line (pt 176 32)(pt 160 32)(line_width 3))
	)
	(drawing
		(rectangle (rect 16 16 160 240)(line_width 1))
	)
)
