/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2006 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 64 64 280 280)
	(text "usb_full_interface_v" (rect 5 0 106 12)(font "Arial" ))
	(text "inst" (rect 8 200 25 212)(font "Arial" ))
	(port
		(pt 0 40)
		(input)
		(text "n_reset" (rect 0 0 36 12)(font "Arial" ))
		(text "n_reset" (rect 21 35 57 47)(font "Arial" ))
		(line (pt 0 40)(pt 16 40)(line_width 1))
	)
	(port
		(pt 0 24)
		(input)
		(text "clk" (rect 0 0 14 12)(font "Arial" ))
		(text "clk" (rect 21 19 35 31)(font "Arial" ))
		(line (pt 0 24)(pt 16 24)(line_width 1))
	)
	(port
		(pt 0 88)
		(input)
		(text "RXF" (rect 0 0 21 12)(font "Arial" ))
		(text "RXF" (rect 21 83 42 95)(font "Arial" ))
		(line (pt 0 88)(pt 16 88)(line_width 1))
	)
	(port
		(pt 0 104)
		(input)
		(text "TXE" (rect 0 0 18 12)(font "Arial" ))
		(text "TXE" (rect 21 99 39 111)(font "Arial" ))
		(line (pt 0 104)(pt 16 104)(line_width 1))
	)
	(port
		(pt 0 176)
		(input)
		(text "single_data_bus" (rect 0 0 79 12)(font "Arial" ))
		(text "single_data_bus" (rect 21 171 100 183)(font "Arial" ))
		(line (pt 0 176)(pt 16 176)(line_width 1))
	)
	(port
		(pt 0 160)
		(input)
		(text "n_wait" (rect 0 0 30 12)(font "Arial" ))
		(text "n_wait" (rect 21 155 51 167)(font "Arial" ))
		(line (pt 0 160)(pt 16 160)(line_width 1))
	)
	(port
		(pt 0 136)
		(input)
		(text "interrupt" (rect 0 0 40 12)(font "Arial" ))
		(text "interrupt" (rect 21 131 61 143)(font "Arial" ))
		(line (pt 0 136)(pt 16 136)(line_width 1))
	)
	(port
		(pt 0 192)
		(input)
		(text "read_req" (rect 0 0 42 12)(font "Arial" ))
		(text "read_req" (rect 21 187 63 199)(font "Arial" ))
		(line (pt 0 192)(pt 16 192)(line_width 1))
	)
	(port
		(pt 0 72)
		(input)
		(text "USB_DATA[7..0]" (rect 24 72 118 86)(font "Arial" (font_size 8)))
		(text "USB_DATA[7..0]" (rect 24 64 118 78)(font "Arial" (font_size 8)))
		(line (pt 0 72)(pt 16 72)(color 0 128 255)(line_width 3))
	)
	(port
		(pt 216 104)
		(output)
		(text "RD" (rect 0 0 16 12)(font "Arial" ))
		(text "RD" (rect 179 99 195 111)(font "Arial" ))
		(line (pt 216 104)(pt 200 104)(line_width 1))
	)
	(port
		(pt 216 120)
		(output)
		(text "WR" (rect 0 0 18 12)(font "Arial" ))
		(text "WR" (rect 177 115 195 127)(font "Arial" ))
		(line (pt 216 120)(pt 200 120)(line_width 1))
	)
	(port
		(pt 216 24)
		(output)
		(text "subadd[6..0]" (rect 0 0 61 12)(font "Arial" ))
		(text "subadd[6..0]" (rect 134 19 195 31)(font "Arial" ))
		(line (pt 216 24)(pt 200 24)(line_width 3))
	)
	(port
		(pt 216 56)
		(output)
		(text "n_write" (rect 0 0 34 12)(font "Arial" ))
		(text "n_write" (rect 161 51 195 63)(font "Arial" ))
		(line (pt 216 56)(pt 200 56)(line_width 1))
	)
	(port
		(pt 216 72)
		(output)
		(text "n_read" (rect 0 0 33 12)(font "Arial" ))
		(text "n_read" (rect 162 67 195 79)(font "Arial" ))
		(line (pt 216 72)(pt 200 72)(line_width 1))
	)
	(port
		(pt 216 88)
		(output)
		(text "n_sync" (rect 0 0 36 12)(font "Arial" ))
		(text "n_sync" (rect 159 83 195 95)(font "Arial" ))
		(line (pt 216 88)(pt 200 88)(line_width 1))
	)
	(port
		(pt 216 160)
		(output)
		(text "busy" (rect 0 0 24 12)(font "Arial" ))
		(text "busy" (rect 171 155 195 167)(font "Arial" ))
		(line (pt 216 160)(pt 200 160)(line_width 1))
	)
	(port
		(pt 216 40)
		(bidir)
		(text "data[7..0]" (rect 0 0 47 12)(font "Arial" ))
		(text "data[7..0]" (rect 148 35 195 47)(font "Arial" ))
		(line (pt 216 40)(pt 200 40)(line_width 3))
	)
	(drawing
		(rectangle (rect 16 16 200 200)(line_width 1))
	)
)
